<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="20.625" y1="33.518" x2="6.223" y2="33.518" width="0" layer="20"/>
<wire x1="6.223" y1="33.518" x2="0" y2="27.295" width="0" layer="20"/>
<wire x1="0" y1="27.295" x2="0" y2="6.223" width="0" layer="20"/>
<wire x1="0" y1="6.223" x2="6.223" y2="0" width="0" layer="20"/>
<wire x1="6.223" y1="0" x2="20.625" y2="0" width="0" layer="20"/>
<wire x1="20.625" y1="0" x2="20.625" y2="33.518" width="0" layer="20"/>
<text>JTAG 10-20</text>
<text>Jason Lopez</text>
</plain>
<libraries>
<library name="AtomBasics">
<packages>
<package name="JTAG-ARM">
<description>20 Pin JTAG Connector (ARM7, ARM9)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JTAG" library="AtomBasics" package="JTAG-ARM" value="">
<attribute name="VALUE"/>
</element>
<element name="JTAGX10" library="SparkFun-Connectors" package="2X5-SHROUDED-NS" value="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JTAG" pad="8"/>
<contactref element="JTAG" pad="6"/>
<contactref element="JTAG" pad="4"/>
<contactref element="JTAGX10" pad="3"/>
<contactref element="JTAGX10" pad="5"/>
<contactref element="JTAGX10" pad="9"/>
</signal>
<signal name="SAM_TCK">
<contactref element="JTAG" pad="9"/>
<contactref element="JTAGX10" pad="4"/>
</signal>
<signal name="SAM_TMS">
<contactref element="JTAG" pad="7"/>
<contactref element="JTAGX10" pad="2"/>
</signal>
<signal name="SAM_TDO">
<contactref element="JTAG" pad="13"/>
<contactref element="JTAGX10" pad="6"/>
</signal>
<signal name="SAM_NSRST">
<contactref element="JTAG" pad="15"/>
<contactref element="JTAGX10" pad="10"/>
</signal>
<signal name="SAM_VTG">
<contactref element="JTAG" pad="1"/>
<contactref element="JTAGX10" pad="1"/>
</signal>
<signal name="SW_SAM_TDI">
<contactref element="JTAG" pad="17"/>
<contactref element="JTAGX10" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
