<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="16.18" y2="0" width="0" layer="20"/>
<wire x1="16.18" y1="0" x2="16.18" y2="20.31" width="0" layer="20"/>
<wire x1="16.18" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<hole x="11.43" y="17.78" drill="1.6"/>
<hole x="11.43" y="2.54" drill="1.6"/>
<text>+5V</text>
<text>D-</text>
<text>D+</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="USB">
<description>&lt;b&gt;USB connector&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-amp" package="USB" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SHIELD">
</signal>
</signals>
</board>
</drawing>
</eagle>
