<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<hole x="42.545" y="3.048" drill="2.2"/>
<hole x="56.007" y="19.05" drill="2.2"/>
<text>Pololu 5V, 5A</text>
<text>Voltage Regulator</text>
<text>D24V50F5</text>
<text>5V</text>
<text>G</text>
<text>G</text>
<hole x="30.734" y="2.794" drill="3.2"/>
<hole x="67.564" y="2.921" drill="3.2"/>
<hole x="67.691" y="29.21" drill="3.2"/>
<hole x="30.734" y="29.083" drill="3.2"/>
<text>5V</text>
<text>G</text>
<text>G</text>
<text>Vin</text>
<text>Vin</text>
<text>5V</text>
<text>G</text>
<text>G</text>
<text>5V</text>
<wire x1="27.813" y1="0.254" x2="70.739" y2="0.254" width="0" layer="20"/>
<wire x1="70.739" y1="0.254" x2="70.739" y2="31.75" width="0" layer="20"/>
<wire x1="70.739" y1="31.75" x2="27.813" y2="31.75" width="0" layer="20"/>
<wire x1="27.813" y1="31.75" x2="27.813" y2="0.254" width="0" layer="20"/>
<text>Vin:</text>
<text>FlthyMiniReg v1</text>
<text>7-36V</text>
<text>5V@5A</text>
<text>Vout:</text>
</plain>
<libraries>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$8" library="con-lstb" package="MA04-1" value="">
<attribute name="VALUE"/>
</element>
<element name="E$12" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$9" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="con-lstb" package="MA05-2" value="">
<attribute name="VALUE"/>
</element>
<element name="E$1" library="adafruit" package="0204/7" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
<signal name="S$5">
</signal>
<signal name="S$7">
</signal>
<signal name="S$2">
</signal>
<signal name="S$6">
</signal>
<signal name="S$8">
</signal>
<signal name="GND">
<contactref element="E$8" pad="3"/>
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="12V">
</signal>
<signal name="5V">
<contactref element="E$3" pad="A"/>
</signal>
<signal name="S$1">
</signal>
<signal name="VIN">
</signal>
</signals>
</board>
</drawing>
</eagle>
