<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="52" y2="0" width="0" layer="20"/>
<wire x1="52" y1="0" x2="52" y2="37.5" width="0" layer="20"/>
<wire x1="52" y1="37.5" x2="0" y2="37.5" width="0" layer="20"/>
<wire x1="0" y1="37.5" x2="0" y2="0" width="0" layer="20"/>
<text>Nest Device
Clemson University</text>
<text>CC1101</text>
<text>MAX3232</text>
<text>X</text>
<text>GND</text>
<hole x="50" y="35.5" drill="1.5"/>
<hole x="2" y="2" drill="1.5"/>
<text>TXD</text>
<text>RXD</text>
<text>RST</text>
<text>TST</text>
<text>VCC</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>3.3V</text>
<text>9V</text>
<text>GND</text>
<hole x="50" y="2" drill="1.5"/>
<hole x="2" y="18.25" drill="1.5"/>
<hole x="26" y="35.5" drill="1.5"/>
<text>P3.0</text>
<hole x="2" y="35.5" drill="1.5"/>
<text>Jeremy Wilder</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5_NOSILK">
</package>
<package name="1X10_NO_SILK">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X06_NO_SILK">
</package>
</packages>
</library>
<library name="msp430">
<packages>
<package name="RGZ48_4P1X4P1">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="abs05">
<packages>
<package name="ABS05">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="msp430" package="RGZ48_4P1X4P1" value="MSP430FR5969_RGZ_48">
<attribute name="MANUFACTURER_PART_NUMBER" value="msp430fr5969_rgz_48"/>
<attribute name="VENDOR" value="Texas Instruments"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="SOT23-5" value="3.3V">
<attribute name="PROD_ID" value="VREG-09872"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805-CAP" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805-CAP" value="470pF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805-CAP" value=".33uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805-CAP" value=".1uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805-CAP" value="9pF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805-CAP" value="9pF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="X1" library="abs05" package="ABS05" value="ABS05-32.768KHZ-9-T">
<attribute name="DIGIKEY" value="535-11897-1-ND"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X5_NOSILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="9+" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MOSFET-PCHANNEL">
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="PRGMR" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="TO220H" value="7809T"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="41"/>
<contactref element="U1" pad="36"/>
<contactref element="U5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="9"/>
<contactref element="9+" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J2" pad="2"/>
<contactref element="PRGMR" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="P1.6">
<contactref element="U1" pad="31"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="P1.7">
<contactref element="U1" pad="32"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="P1.3">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="P2.2">
<contactref element="U1" pad="26"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="P3.6">
<contactref element="U1" pad="29"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="P3.4">
<contactref element="U1" pad="27"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="P2.6">
<contactref element="J4" pad="4"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="P2.5">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="IC2" pad="3"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U5" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$23">
</signal>
<signal name="A">
<contactref element="U1" pad="46"/>
<contactref element="X1" pad="A"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="B">
<contactref element="U1" pad="45"/>
<contactref element="X1" pad="B"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$24">
</signal>
<signal name="P3.5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="DRAIN">
<contactref element="9+" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="RFID-RX">
<contactref element="J4" pad="10"/>
</signal>
<signal name="RFID-TX">
<contactref element="J4" pad="8"/>
</signal>
<signal name="3.3V">
<contactref element="U5" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="37"/>
<contactref element="J1" pad="1"/>
<contactref element="J4" pad="6"/>
<contactref element="PRGMR" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="MOSFET">
<contactref element="U1" pad="4"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="25"/>
<contactref element="PRGMR" pad="6"/>
</signal>
<signal name="TEST">
<contactref element="U1" pad="22"/>
<contactref element="PRGMR" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="23"/>
<contactref element="PRGMR" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="24"/>
<contactref element="PRGMR" pad="5"/>
</signal>
<signal name="TDI">
<contactref element="U1" pad="13"/>
</signal>
<signal name="TMS">
<contactref element="U1" pad="14"/>
</signal>
<signal name="TCK">
<contactref element="U1" pad="15"/>
</signal>
<signal name="TDO">
<contactref element="U1" pad="12"/>
</signal>
<signal name="P3.2">
<contactref element="U1" pad="6"/>
</signal>
<signal name="P3.3">
<contactref element="U1" pad="7"/>
</signal>
<signal name="P1.4">
<contactref element="U1" pad="10"/>
</signal>
<signal name="P4.0">
<contactref element="U1" pad="16"/>
</signal>
<signal name="P4.1">
<contactref element="U1" pad="17"/>
</signal>
<signal name="P!.3">
</signal>
</signals>
</board>
</drawing>
</eagle>
