<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="45.72" x2="0" y2="5.08" width="0" layer="20"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="40.64" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="40.64" y1="5.08" x2="40.64" y2="45.72" width="0" layer="20"/>
<wire x1="40.64" y1="45.72" x2="35.56" y2="50.8" width="0" layer="20" curve="90"/>
<wire x1="35.56" y1="50.8" x2="5.08" y2="50.8" width="0" layer="20"/>
<wire x1="5.08" y1="50.8" x2="0" y2="45.72" width="0" layer="20" curve="90"/>
<text>TEST
MODE</text>
<text>RUN
MODE</text>
<text>TL4G3 PROGRAMMER REV C</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.3 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint&lt;/h3&gt;
Pins are staggered 0.005" off center to lock pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H1" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H2" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H3" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="H4" library="holes" package="3,3" value="MOUNT-HOLE3.3"/>
<element name="J1" library="SparkFun-Connectors" package="1X09" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X09" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="J6" library="SparkFun-Connectors" package="2X5-SHROUDED-NS" value="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="12k">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="12k">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT4904">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08052"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08052"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="6"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="GND">
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J6" pad="8"/>
<contactref element="J6" pad="7"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="9"/>
</signal>
<signal name="RTS">
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="DTR">
<contactref element="R1" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="J3" pad="2"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="TX">
<contactref element="J3" pad="3"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="TEST">
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="EN">
<contactref element="J6" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="IO0">
<contactref element="J6" pad="10"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
