<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="5.08" x2="0" y2="63.5" width="1.27" layer="20"/>
<wire x1="5.08" y1="68.58" x2="63.5" y2="68.58" width="1.27" layer="20"/>
<wire x1="68.58" y1="63.5" x2="68.58" y2="5.08" width="1.27" layer="20"/>
<wire x1="63.5" y1="0" x2="5.08" y2="0" width="1.27" layer="20"/>
<wire x1="0" y1="63.5" x2="5.08" y2="68.58" width="1.27" layer="20" curve="-90"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="1.27" layer="20" curve="90"/>
<wire x1="68.58" y1="5.08" x2="63.5" y2="0" width="1.27" layer="20" curve="-90"/>
<wire x1="68.58" y1="5.08" x2="63.5" y2="0" width="1.27" layer="20" curve="-90"/>
<wire x1="68.58" y1="63.5" x2="63.5" y2="68.58" width="1.27" layer="20" curve="90"/>
</plain>
<libraries>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCJ0202">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
</packages>
</library>
<library name="113990105">
<packages>
<package name="SEEED_113990105">
</package>
</packages>
</library>
<library name="Switch">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Switches&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="2-1825910-7">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE05W">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="con-jack" package="DCJ0202" value="DCJ0202">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="ESP8266" library="113990105" package="SEEED_113990105" value="113990105">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" An open-source firmware and development kit that helps you to Prototype your IOT product within a few Lua script lines "/>
<attribute name="ESP8266" value=""/>
<attribute name="MF" value="Seeed Technology"/>
<attribute name="MP" value="NodeMCU v2"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q1" library="transistor-power" package="D2PACK" value="IRF3704S">
<attribute name="NAME"/>
</element>
<element name="Q2" library="transistor-power" package="D2PACK" value="IRF3704S">
<attribute name="NAME"/>
</element>
<element name="Q3" library="transistor-power" package="D2PACK" value="IRF3704S">
<attribute name="NAME"/>
</element>
<element name="Q4" library="transistor-power" package="D2PACK" value="IRF3704S">
<attribute name="NAME"/>
</element>
<element name="J2" library="con-lsta" package="FE05W" value="RGBW1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="SW1" library="Switch" package="2-1825910-7" value="2-1825910-7">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="450-1642-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity ALCOSWITCH Switches"/>
<attribute name="MPN" value="2-1825910-7"/>
</element>
<element name="SW2" library="Switch" package="2-1825910-7" value="2-1825910-7">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="450-1642-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity ALCOSWITCH Switches"/>
<attribute name="MPN" value="2-1825910-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="Switch" package="2-1825910-7" value="2-1825910-7">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="450-1642-ND"/>
<attribute name="MANUFACTURER" value="TE Connectivity ALCOSWITCH Switches"/>
<attribute name="MPN" value="2-1825910-7"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="eagle-ltspice" package="C1005" value="">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="eagle-ltspice" package="C1005" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="TO252" value="7805DT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="33">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08270"/>
<attribute name="VALUE" value="33"/>
</element>
</elements>
<signals>
<signal name="W-MAIN">
<contactref element="ESP8266" pad="J2_8"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="G-MAIN">
<contactref element="ESP8266" pad="J2_10"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="B-MAIN">
<contactref element="ESP8266" pad="J2_9"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="R-MAIN">
<contactref element="ESP8266" pad="J2_11"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="5VDC">
<contactref element="ESP8266" pad="J1_15"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="B-IN">
<contactref element="Q2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="G-IN">
<contactref element="Q3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="R-IN">
<contactref element="Q4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="R-OUT">
<contactref element="Q4" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="G-OUT">
<contactref element="J2" pad="3"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="B-OUT">
<contactref element="Q2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="W-OUT">
<contactref element="Q1" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="12VDC">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="ESP8266" pad="J1_13"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="W-CTL">
<contactref element="SW3" pad="1"/>
<contactref element="SW3" pad="2"/>
<contactref element="ESP8266" pad="J2_2"/>
<contactref element="R11" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="M-CTL">
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="ESP8266" pad="J2_3"/>
<contactref element="R9" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="3.3VDC">
<contactref element="ESP8266" pad="J2_15"/>
<contactref element="ESP8266" pad="J2_6"/>
<contactref element="SW3" pad="4"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="4"/>
<contactref element="SW3" pad="3"/>
<contactref element="ESP8266" pad="J1_11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ESP8266" pad="J1_10"/>
<contactref element="ESP8266" pad="J1_14"/>
<contactref element="ESP8266" pad="J2_14"/>
<contactref element="ESP8266" pad="J2_7"/>
<contactref element="R11" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="W-IN">
<contactref element="Q1" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="C"/>
<contactref element="R13" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
