<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="65" y2="3" width="0" layer="20" curve="90"/>
<wire x1="65" y1="3" x2="65" y2="53" width="0" layer="20"/>
<wire x1="65" y1="53" x2="62" y2="56" width="0" layer="20" curve="90"/>
<wire x1="62" y1="56" x2="3" y2="56" width="0" layer="20"/>
<wire x1="3" y1="56" x2="0" y2="53" width="0" layer="20" curve="90"/>
<wire x1="0" y1="53" x2="0" y2="3" width="0" layer="20"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<text>TOP</text>
<text>BOTTOM</text>
<text>+5v</text>
<text>+5v</text>
<text>+5v</text>
<text>1W-A</text>
<text>SDA</text>
<text>3V3</text>
<text>Gnd</text>
<text>1W-B</text>
<text>Gnd</text>
<text>SDA</text>
<text>+5V</text>
<text>IO-A4</text>
<text>Gnd</text>
<text>IO-A6</text>
<text>IO-A2</text>
<text>IO-A0</text>
<text>Gnd</text>
<text>Gnd</text>
<text>CH3-B</text>
<text>CH1-B</text>
<text>CH3-A</text>
<text>CH1-A</text>
<text>Gnd</text>
<text>Multi-IO Board</text>
<text>Rev 1.0
AGW Nov 2017</text>
</plain>
<libraries>
<library name="FLYFISH">
<packages>
<package name="PIN_20X2">
</package>
<package name="SOIC8">
</package>
<package name="PIN_W_2">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt; 8 SO&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOIC127P1030X265-28N">
<description>&lt;b&gt;28-Lead Plastic Small Outline (SO) - Wide 7.50mm Body (SOIC)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="6-LEAD-TSOC">
<description>&lt;b&gt;6-Lead-TSOC&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOIC127P1032X265-16N">
<description>&lt;b&gt;DS1210S 16-pin SOIC (300-mil)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOIC127P600X175-14N">
<description>&lt;b&gt;14-Lead(SL) SOIC&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="TSOT23_6-LEAD">
<description>&lt;b&gt;TSOT23 6 LEAD CASE 419AG-01&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SC75_INFINEON">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; Reflow soldering&lt;p&gt;
INFINEON, www.infineon.com/cmc_upload/0/000/010/257/eh_db_5b.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jump-0r-smd">
<description>Soldering jumper and bridges</description>
<packages>
<package name="A0R-JMP">
<description>&lt;b&gt;0R Jumper Variant A&lt;/b&gt;&lt;p&gt;
chip 0805</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD80C">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CH291-1220LF">
<description>&lt;b&gt;Battery Holder, SMT, 12mm&lt;/b&gt;&lt;p&gt;
multicomp PART NO. CH291-1220LF&lt;br&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/1505860.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="smd-special">
<description>&lt;b&gt;Special SMD Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMS-004">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="FLYFISH" package="PIN_20X2" value="PIN20X2">
<attribute name="VALUE"/>
</element>
<element name="U1" library="FLYFISH" package="SOIC8" value="EEPROM24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="CFG" library="FLYFISH" package="PIN_W_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="IC1" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="ISO1541D">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="2.5 kVrms Isolated Unidirectional Clock, Bidirectional I2C Isolators"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ISO1541D"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="8253075"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC3" library="SamacSys_Parts" package="SOIC127P1030X265-28N" value="MCP23017-E_SO">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value="70046137"/>
<attribute name="DESCRIPTION" value="16-bit I/O Expander,I2C,MCP23017-E/SO"/>
<attribute name="HEIGHT" value="2.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP23017-E/SO"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="0403816P"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="DS2482S-100+">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="Single-Channel 1-Wire Master"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DS2482S-100+"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7327551"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="C2" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-fet" package="SC75_INFINEON" value="BSA223SP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="JMP1" library="jump-0r-smd" package="A0R-JMP" value="0R-JUMPA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JMP2" library="jump-0r-smd" package="A0R-JMP" value="0R-JUMPA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="JMP3" library="jump-0r-smd" package="A0R-JMP" value="0R-JUMPA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="2X05/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="SamacSys_Parts" package="6-LEAD-TSOC" value="DS9503P+">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="I.C. DS9503P Maxim DS9503P+ ESD Protection Diode, 6-Pin TSOC"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DS9503P+"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="5402906"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC5" library="SamacSys_Parts" package="6-LEAD-TSOC" value="DS9503P+">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="I.C. DS9503P Maxim DS9503P+ ESD Protection Diode, 6-Pin TSOC"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DS9503P+"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="5402906"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC6" library="SamacSys_Parts" package="SOIC127P600X175-8N" value="DS2482S-100+">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="Single-Channel 1-Wire Master"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DS2482S-100+"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7327551"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="C4" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-fet" package="SC75_INFINEON" value="BSA223SP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="JMP4" library="jump-0r-smd" package="A0R-JMP" value="0R-JUMPA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="SamacSys_Parts" package="SOIC127P1032X265-16N" value="DS3231M+">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="Real Time Clock 5+/-ppm RTC"/>
<attribute name="HEIGHT" value="2.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DS3231M+"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC8" library="SamacSys_Parts" package="SOIC127P600X175-14N" value="MCP3428-E_SL">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value="70047321"/>
<attribute name="DESCRIPTION" value="16-bit delta-sigma ADC, quad channel"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP3428-E/SL"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7037945"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC9" library="SamacSys_Parts" package="SOIC127P600X175-14N" value="MCP3428-E_SL">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value="70047321"/>
<attribute name="DESCRIPTION" value="16-bit delta-sigma ADC, quad channel"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP3428-E/SL"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7037945"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="C5" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C6" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C7" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="R14" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SamacSys_Parts" package="TSOT23_6-LEAD" value="FDC6301N">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="ON SEMICONDUCTOR/FAIRCHILD - FDC6301N.. - MOSFET, NN CH, 25V, 0.22A, SSOT6"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Fairchild Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FDC6301N"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7390155P"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R16" library="resistor" package="M0805" value="2k2">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R17" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="diode" package="SOD80C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R66" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R67" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R68" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R69" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R70" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R71" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R62" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R63" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G1" library="battery" package="CH291-1220LF" value="CH291-1220LF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="smd-special" package="SMS-004" value="SWS004">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R73" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R74" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R75" library="resistor" package="M0805" value="2k2">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R76" library="resistor" package="R0603" value="220">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R77" library="resistor" package="R0603" value="220">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R78" library="resistor" package="R0603" value="220">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R79" library="resistor" package="R0603" value="220">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SamacSys_Parts" package="TSOT23_6-LEAD" value="FDC6301N">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="ON SEMICONDUCTOR/FAIRCHILD - FDC6301N.. - MOSFET, NN CH, 25V, 0.22A, SSOT6"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Fairchild Semiconductor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FDC6301N"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7390155P"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R80" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R81" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R82" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R83" library="resistor" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="SMC_C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="SMC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="SMC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="SMC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="SMC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="SMC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ2" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ3" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="SJ4" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="C24" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="R84" library="resistor" package="R0603" value="100">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R85" library="resistor" package="R0603" value="100">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R86" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R87" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R88" library="resistor" package="R0603" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R89" library="resistor" package="R0603" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R90" library="resistor" package="R0603" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="CFG" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="K1" pad="9"/>
<contactref element="K1" pad="25"/>
<contactref element="K1" pad="39"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="14"/>
<contactref element="K1" pad="20"/>
<contactref element="K1" pad="30"/>
<contactref element="K1" pad="34"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC2" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="IC3" pad="17"/>
<contactref element="JMP1" pad="1"/>
<contactref element="JMP2" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="JMP3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R9" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="IC6" pad="7"/>
<contactref element="JMP4" pad="1"/>
<contactref element="IC8" pad="2"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC9" pad="2"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="14"/>
<contactref element="IC9" pad="12"/>
<contactref element="IC9" pad="14"/>
<contactref element="IC8" pad="12"/>
<contactref element="IC7" pad="13"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="D8" pad="A"/>
<contactref element="R41" pad="1"/>
<contactref element="D7" pad="A"/>
<contactref element="R40" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="R39" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="R38" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="R37" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="R36" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="R35" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="12"/>
<contactref element="JP1" pad="12"/>
<contactref element="JP2" pad="2"/>
<contactref element="G1" pad="-"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="6"/>
<contactref element="C16" pad="-"/>
<contactref element="C17" pad="-"/>
<contactref element="C18" pad="-"/>
<contactref element="C19" pad="-"/>
<contactref element="C20" pad="-"/>
<contactref element="C21" pad="-"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="SJ4" pad="2"/>
<contactref element="SJ3" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="7"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC7" pad="12"/>
<contactref element="IC7" pad="11"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC7" pad="9"/>
<contactref element="IC9" pad="5"/>
<contactref element="IC8" pad="5"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="SJ5" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="17"/>
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="IC7" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="R16" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="R80" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="R83" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="CFG" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="K1" pad="2"/>
<contactref element="K1" pad="4"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC3" pad="18"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC3" pad="9"/>
<contactref element="R66" pad="2"/>
<contactref element="R67" pad="2"/>
<contactref element="R68" pad="2"/>
<contactref element="R69" pad="2"/>
<contactref element="R70" pad="2"/>
<contactref element="R71" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="JP2" pad="11"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="11"/>
<contactref element="JP2" pad="1"/>
<contactref element="R72" pad="2"/>
<contactref element="R75" pad="2"/>
<contactref element="R74" pad="2"/>
<contactref element="R73" pad="2"/>
<contactref element="JP3" pad="9"/>
<contactref element="JP3" pad="10"/>
<contactref element="R81" pad="2"/>
<contactref element="R82" pad="2"/>
<contactref element="C21" pad="+"/>
<contactref element="C16" pad="+"/>
<contactref element="C20" pad="+"/>
<contactref element="C19" pad="+"/>
<contactref element="C18" pad="+"/>
<contactref element="C17" pad="+"/>
<contactref element="IC9" pad="6"/>
<contactref element="IC8" pad="6"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="R86" pad="2"/>
<contactref element="R87" pad="2"/>
<contactref element="R89" pad="2"/>
<contactref element="R88" pad="2"/>
<contactref element="R90" pad="2"/>
</signal>
<signal name="SDA_5V">
<contactref element="IC1" pad="7"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC9" pad="7"/>
<contactref element="Q3" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="JP3" pad="8"/>
<contactref element="IC8" pad="7"/>
</signal>
<signal name="SCL_5V">
<contactref element="IC1" pad="6"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC9" pad="8"/>
<contactref element="Q3" pad="6"/>
<contactref element="R17" pad="1"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="6"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="3"/>
<contactref element="IC7" pad="15"/>
<contactref element="IC1" pad="2"/>
<contactref element="K1" pad="3"/>
<contactref element="Q3" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="4"/>
<contactref element="IC7" pad="16"/>
<contactref element="IC1" pad="3"/>
<contactref element="K1" pad="5"/>
<contactref element="Q3" pad="5"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="IO-A0">
<contactref element="IC3" pad="21"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="IO-A1">
<contactref element="IC3" pad="22"/>
<contactref element="R50" pad="2"/>
</signal>
<signal name="IO-A2">
<contactref element="IC3" pad="23"/>
<contactref element="R51" pad="2"/>
</signal>
<signal name="IO-A3">
<contactref element="IC3" pad="24"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="IO-A4">
<contactref element="IC3" pad="25"/>
<contactref element="R53" pad="2"/>
</signal>
<signal name="IO-A5">
<contactref element="IC3" pad="26"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="IO-A6">
<contactref element="IC3" pad="27"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="IO-A7">
<contactref element="IC3" pad="28"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="IO-B0">
<contactref element="IC3" pad="1"/>
<contactref element="R72" pad="1"/>
<contactref element="S1" pad="8"/>
</signal>
<signal name="IO-B1">
<contactref element="IC3" pad="2"/>
<contactref element="R73" pad="1"/>
<contactref element="S1" pad="7"/>
</signal>
<signal name="IO-B2">
<contactref element="IC3" pad="3"/>
<contactref element="S1" pad="6"/>
<contactref element="R74" pad="1"/>
</signal>
<signal name="IO-B3">
<contactref element="IC3" pad="4"/>
<contactref element="S1" pad="5"/>
<contactref element="R75" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC3" pad="16"/>
<contactref element="JMP2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JMP2" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC2" pad="8"/>
<contactref element="JMP3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="1"/>
<contactref element="JMP3" pad="3"/>
</signal>
<signal name="IO-B4">
<contactref element="IC3" pad="5"/>
<contactref element="R76" pad="2"/>
</signal>
<signal name="IO-B5">
<contactref element="IC3" pad="6"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="IO-B6">
<contactref element="IC3" pad="7"/>
<contactref element="R78" pad="2"/>
</signal>
<signal name="IO-B7">
<contactref element="IC3" pad="8"/>
<contactref element="R79" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="IO-A0-OUT">
<contactref element="R11" pad="1"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="IC6" pad="6"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R12" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="IC6" pad="8"/>
<contactref element="JMP4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R13" pad="1"/>
<contactref element="JMP4" pad="3"/>
</signal>
<signal name="RET_B">
<contactref element="JP3" pad="3"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="IC5" pad="6"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="RET_A">
<contactref element="IC5" pad="5"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC7" pad="14"/>
<contactref element="G1" pad="+"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="CLK_32KHZ">
<contactref element="IC7" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="K1" pad="29"/>
</signal>
<signal name="CLK_INT">
<contactref element="IC7" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="K1" pad="31"/>
</signal>
<signal name="CLK_RST">
<contactref element="IC7" pad="4"/>
<contactref element="K1" pad="33"/>
</signal>
<signal name="N$17">
<contactref element="K1" pad="28"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$23">
<contactref element="K1" pad="27"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="IO-A7-OUT">
<contactref element="R26" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="IO-A5-OUT">
<contactref element="R24" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="IO-A3-OUT">
<contactref element="R22" pad="1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="IO-A1-OUT">
<contactref element="R20" pad="1"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="CH4_A">
<contactref element="IC8" pad="13"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="CH3_A">
<contactref element="IC8" pad="11"/>
<contactref element="R62" pad="2"/>
</signal>
<signal name="CH4_B">
<contactref element="IC9" pad="13"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="CH3_B">
<contactref element="IC9" pad="11"/>
<contactref element="R58" pad="2"/>
</signal>
<signal name="CH2_B">
<contactref element="IC9" pad="3"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="CH1_B">
<contactref element="IC9" pad="1"/>
<contactref element="R60" pad="2"/>
</signal>
<signal name="CH2_A">
<contactref element="IC8" pad="3"/>
<contactref element="R63" pad="2"/>
</signal>
<signal name="CH1_A">
<contactref element="IC8" pad="1"/>
<contactref element="R64" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="15"/>
<contactref element="JMP1" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="JMP1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R20" pad="2"/>
<contactref element="R50" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R51" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R22" pad="2"/>
<contactref element="R52" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="D4" pad="C"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R53" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="D5" pad="C"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="R54" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="D6" pad="C"/>
<contactref element="R69" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R55" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="D7" pad="C"/>
<contactref element="R70" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R26" pad="2"/>
<contactref element="R56" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="D8" pad="C"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="IO-A6-OUT">
<contactref element="R25" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="IO-A4-OUT">
<contactref element="R23" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="IO-A2-OUT">
<contactref element="R21" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$21">
<contactref element="R42" pad="2"/>
<contactref element="R57" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="R86" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R58" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R59" pad="1"/>
<contactref element="R44" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R45" pad="2"/>
<contactref element="R60" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="R90" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R61" pad="1"/>
<contactref element="R46" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="R30" pad="2"/>
<contactref element="R88" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R47" pad="2"/>
<contactref element="R62" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="R89" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R63" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R49" pad="2"/>
<contactref element="R64" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="R87" pad="1"/>
</signal>
<signal name="CH1_A_OUT">
<contactref element="R49" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="CH2_A_OUT">
<contactref element="R48" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="CH3_A_OUT">
<contactref element="R47" pad="1"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="CH4_A_OUT">
<contactref element="R46" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="CH1_B_OUT">
<contactref element="R45" pad="1"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="CH2_B_OUT">
<contactref element="R44" pad="1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="CH3_B_OUT">
<contactref element="R43" pad="1"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="CH4_B_OUT">
<contactref element="R42" pad="1"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="1W_B">
<contactref element="Q1" pad="2"/>
<contactref element="R84" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="1W_A">
<contactref element="Q2" pad="2"/>
<contactref element="R85" pad="1"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="LED1" pad="A"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="LED2" pad="A"/>
<contactref element="R77" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="LED3" pad="A"/>
<contactref element="R78" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="LED4" pad="A"/>
<contactref element="R79" pad="1"/>
</signal>
<signal name="INTA_5V">
<contactref element="Q4" pad="4"/>
<contactref element="R82" pad="1"/>
<contactref element="IC3" pad="20"/>
</signal>
<signal name="INTB_5V">
<contactref element="Q4" pad="6"/>
<contactref element="R81" pad="1"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="INTA">
<contactref element="Q4" pad="2"/>
<contactref element="R80" pad="2"/>
<contactref element="K1" pad="37"/>
</signal>
<signal name="INTB">
<contactref element="Q4" pad="5"/>
<contactref element="R83" pad="2"/>
<contactref element="K1" pad="38"/>
</signal>
<signal name="N$14">
<contactref element="IC8" pad="9"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC8" pad="10"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="SJ2" pad="1"/>
<contactref element="IC9" pad="9"/>
</signal>
<signal name="N$48">
<contactref element="IC9" pad="10"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="IO_A">
<contactref element="R85" pad="2"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="IO_B">
<contactref element="R84" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="IC4" pad="6"/>
<contactref element="JP3" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
