<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="12.29729375" y1="55.87" x2="1.571084375" y2="55.87" width="0" layer="20"/>
<wire x1="1.571084375" y1="55.87" x2="-3.81" y2="50.488915625" width="0" layer="20" curve="90"/>
<wire x1="-3.81" y1="50.488915625" x2="-3.81" y2="36.1596125" width="0" layer="20"/>
<wire x1="-3.81" y1="36.1596125" x2="1.8696125" y2="30.48" width="0" layer="20" curve="90"/>
<wire x1="1.8696125" y1="30.48" x2="12.289915625" y2="30.48" width="0" layer="20"/>
<wire x1="12.289915625" y1="30.48" x2="17.45" y2="35.640084375" width="0" layer="20" curve="90"/>
<wire x1="17.45" y1="35.640084375" x2="17.45" y2="50.71729375" width="0" layer="20"/>
<wire x1="17.45" y1="50.71729375" x2="12.29729375" y2="55.87" width="0" layer="20" curve="90"/>
<hole x="13.335" y="34.29" drill="3.2"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="2X3">
</package>
<package name="1X08_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BUTTON" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="FLEX" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="LEDS" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="BUTTON" pad="1"/>
<contactref element="LEDS" pad="1"/>
<contactref element="LEDS" pad="2"/>
</signal>
<signal name="LED1">
<contactref element="JP1" pad="3"/>
<contactref element="LEDS" pad="5"/>
</signal>
<signal name="LED2">
<contactref element="JP1" pad="4"/>
<contactref element="LEDS" pad="6"/>
</signal>
<signal name="FLEX1">
<contactref element="JP1" pad="5"/>
<contactref element="FLEX" pad="1"/>
</signal>
<signal name="FLEX2">
<contactref element="JP1" pad="6"/>
<contactref element="FLEX" pad="3"/>
</signal>
<signal name="FLEX3">
<contactref element="JP1" pad="7"/>
<contactref element="FLEX" pad="5"/>
</signal>
<signal name="VIN">
<contactref element="LEDS" pad="3"/>
<contactref element="LEDS" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="R3">
<contactref element="FLEX" pad="6"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="R2">
<contactref element="FLEX" pad="4"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="R1">
<contactref element="FLEX" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="BTN">
<contactref element="BUTTON" pad="2"/>
<contactref element="JP1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
