<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="-0.15833125" y1="12.29808125" x2="17.406928125" y2="12.21295625" width="0" layer="20"/>
<wire x1="17.406928125" y1="12.21295625" x2="17.4493375" y2="24.493403125" width="0" layer="20"/>
<wire x1="17.4493375" y1="24.493403125" x2="0.115925" y2="24.578528125" width="0" layer="20"/>
<wire x1="0.115925" y1="24.578528125" x2="-0.15833125" y2="12.29808125" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED10MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D2" library="SparkFun-LED" package="LED10MM" value="LED"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="QX5252F"/>
<element name="SOLARPANEL" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="BATT" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="L2" library="eagle-ltspice" package="0204/7" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="L"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="SOLARPANEL" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="BATT" pad="1"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="4"/>
<contactref element="D2" pad="A"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="SOLARPANEL" pad="2"/>
<contactref element="BATT" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="D2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
