<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.42" y2="0" width="0" layer="20"/>
<wire x1="58.42" y1="0" x2="58.42" y2="26.67" width="0" layer="20"/>
<wire x1="58.42" y1="26.67" x2="0" y2="26.67" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0" layer="20"/>
<text>RIKKI A500+ VIDEO HYBRID BLINKY</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="a500plusvideohybrid">
<packages>
<package name="1X22_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -22 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:22&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_22&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SOP65P640X120-20N">
</package>
<package name="LED-0805">
<description>&lt;h3&gt;LED 0805 SMT&lt;/h3&gt;

0805, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: ? x ?&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="J1" library="a500plusvideohybrid" package="1X22_LONGPADS" value=""/>
<element name="U1" library="a500plusvideohybrid" package="SOP65P640X120-20N" value="TLC59211IPWR">
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="09R6482"/>
<attribute name="MPN" value="TLC59211IPWR"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="PROD_ID" value="CAP-08469"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="4K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="8K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="470R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="390R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="2K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="PROD_ID" value="CAP-08469"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="4K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="8K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="470R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="390R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="2K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="PROD_ID" value="CAP-08469"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="4K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="8K">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="470R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="390R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="0805" value="75R">
<attribute name="PROD_ID" value=" "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT3904">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="U2" library="a500plusvideohybrid" package="SOP65P640X120-20N" value="TLC59211IPWR">
<attribute name="OC_NEWARK" value="09R6482"/>
<attribute name="MPN" value="TLC59211IPWR"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="PACKAGE" value="TSSOP-20"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R27" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R28" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R29" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R30" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R31" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R32" library="SparkFun-Resistors" package="0805" value="150R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R33" library="SparkFun-Resistors" package="0805" value="80R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R34" library="SparkFun-Resistors" package="0805" value="80R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R35" library="SparkFun-Resistors" package="0805" value="80R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R36" library="SparkFun-Resistors" package="0805" value="80R">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="D1" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KRKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KRKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KRKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KRKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KGKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KGKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KGKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171KGKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171TBKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171TBKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171TBKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="a500plusvideohybrid" package="LED-0805" value="LTST-C171TBKT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="21"/>
<contactref element="J1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="20"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D9" pad="A"/>
<contactref element="D10" pad="A"/>
<contactref element="D11" pad="A"/>
<contactref element="D12" pad="A"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="22"/>
<contactref element="J1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="9"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="DR3">
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="DR2">
<contactref element="J1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="DR1">
<contactref element="J1" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="DR0">
<contactref element="J1" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="DG3">
<contactref element="J1" pad="8"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="DG2">
<contactref element="J1" pad="9"/>
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="DG1">
<contactref element="J1" pad="10"/>
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="DG0">
<contactref element="J1" pad="11"/>
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DB3">
<contactref element="J1" pad="13"/>
<contactref element="R17" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="DB2">
<contactref element="J1" pad="14"/>
<contactref element="R18" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="DB1">
<contactref element="J1" pad="15"/>
<contactref element="R19" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="DB0">
<contactref element="J1" pad="16"/>
<contactref element="R20" pad="1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="R">
<contactref element="J1" pad="7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="G">
<contactref element="J1" pad="12"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="B">
<contactref element="J1" pad="17"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="CSYNC">
<contactref element="J1" pad="18"/>
</signal>
<signal name="COMP">
<contactref element="J1" pad="19"/>
</signal>
<signal name="SYNC">
<contactref element="J1" pad="20"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R9" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="Q2" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R17" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="Q3" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="LG0">
<contactref element="U1" pad="19"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="LG1">
<contactref element="U1" pad="18"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="LG2">
<contactref element="U1" pad="17"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="LG3">
<contactref element="U1" pad="16"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="LR0">
<contactref element="U1" pad="15"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="LR1">
<contactref element="U1" pad="14"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="LR2">
<contactref element="U1" pad="13"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="LR3">
<contactref element="U1" pad="12"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="LB0">
<contactref element="U2" pad="19"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="LB1">
<contactref element="U2" pad="18"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="LB2">
<contactref element="U2" pad="17"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="LB3">
<contactref element="U2" pad="16"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R25" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="R26" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="R27" pad="2"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$17">
<contactref element="R28" pad="2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="R29" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$18">
<contactref element="R30" pad="2"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="R31" pad="2"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="N$22">
<contactref element="R32" pad="2"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="N$24">
<contactref element="R33" pad="2"/>
<contactref element="D9" pad="C"/>
</signal>
<signal name="N$26">
<contactref element="R34" pad="2"/>
<contactref element="D10" pad="C"/>
</signal>
<signal name="N$28">
<contactref element="R35" pad="2"/>
<contactref element="D11" pad="C"/>
</signal>
<signal name="N$30">
<contactref element="R36" pad="2"/>
<contactref element="D12" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
