<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0402-TIGHT">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO_JACK_0.25&quot;_TRS_PTH_RA">
<description>&lt;h3&gt;Right Angle -1/4" Stereo Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Components/General/JP-611%20DD.jpg”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;AUDIO_JACK_TRS_0.25"_PTH_RA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BC9VPC">
<description>&lt;h3&gt;9V Battery Holder (Open) - PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Area: 2.15"x1.20"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.memoryprotectiondevices.com/datasheets/BC9VPC-datasheet.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BC9VPC&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="POT-PTH-ALPS">
<description>&lt;h3&gt;9mm Square Rotary Potentiometer - PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/Linear-Trimpot.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-12417"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-TIGHT" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-14848"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="200mA/100V/1V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="200mA/100V/1V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="200mA/100V/1V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="AUDIO_JACK_0.25&quot;_TRS_PTH_RA" value="AUDIO_JACK_TRS_0.25&quot;_PTH_RA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12339"/>
<attribute name="SF_ID" value="COM-11144"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="BC9VPC" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-10855"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="AUDIO_JACK_0.25&quot;_TRS_PTH_RA" value="AUDIO_JACK_TRS_0.25&quot;_PTH_RA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-12339"/>
<attribute name="SF_ID" value="COM-11144"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="200mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="200mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="SparkFun-Resistors" package="POT-PTH-ALPS" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09177"/>
<attribute name="SF_SKU" value="COM-09288"/>
<attribute name="VALUE"/>
</element>
<element name="VR2" library="SparkFun-Resistors" package="POT-PTH-ALPS" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09177"/>
<attribute name="SF_SKU" value="COM-09288"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="Q1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="Q2" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="VR1" pad="P$1"/>
</signal>
<signal name="3.3V">
<contactref element="VR1" pad="P$3"/>
<contactref element="R2" pad="P$1"/>
<contactref element="VR2" pad="P$3"/>
<contactref element="J3" pad="SLEEVE"/>
<contactref element="J3" pad="SLEEVE-NORM"/>
<contactref element="J2" pad="V-"/>
<contactref element="J1" pad="SLEEVE"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="1"/>
<contactref element="VR2" pad="P$1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="V+"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="TIP"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="RING"/>
<contactref element="J1" pad="TIP-NORM"/>
<contactref element="J1" pad="RING-NORM"/>
</signal>
<signal name="N$12">
<contactref element="J3" pad="TIP"/>
<contactref element="VR2" pad="P$2"/>
<contactref element="J3" pad="RING"/>
<contactref element="J3" pad="RING-NORM"/>
<contactref element="J3" pad="TIP-NORM"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
