<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="8.39" x2="0" y2="0.5" width="0" layer="20"/>
<wire x1="0" y1="0.5" x2="0.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.5" y1="0" x2="12.2" y2="0" width="0" layer="20"/>
<wire x1="12.2" y1="0" x2="12.7" y2="0.5" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="0.5" x2="12.7" y2="8.39" width="0" layer="20"/>
<wire x1="12.7" y1="8.39" x2="12.2" y2="8.89" width="0" layer="20" curve="90"/>
<wire x1="12.2" y1="8.89" x2="0.5" y2="8.89" width="0" layer="20"/>
<wire x1="0.5" y1="8.89" x2="0" y2="8.39" width="0" layer="20" curve="90"/>
<text>VCC</text>
<text>D-</text>
<text>D+</text>
<text>ID</text>
<text>GND</text>
</plain>
<libraries>
<library name="eugen">
<packages>
<package name="MICRO-B-DIP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eugen" package="MICRO-B-DIP" value="MICRO-B-DIP"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="D+"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="ID"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="4"/>
<contactref element="U$2" pad="D-"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="5"/>
<contactref element="U$2" pad="VCC"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
