<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="43.18" width="0" layer="20"/>
<wire x1="35.56" y1="43.18" x2="0" y2="43.17" width="0" layer="20"/>
<wire x1="0" y1="43.17" x2="0" y2="0" width="0" layer="20"/>
<text>Encoder Rev 1.10</text>
<text>CC0 1.0 Universal</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ENCODER_LED_3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
<library name="PJS">
<packages>
<package name="3.2-MOUNT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="82"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="150"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="82"/>
<element name="SW2" library="SparkFun-Electromechanical" package="ENCODER_LED_3" value="SPARKFUN-COM-10982"/>
<element name="J1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="MT1" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
<element name="MT2" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
<element name="MT3" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
<element name="MT4" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
<element name="MT5" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
</elements>
<signals>
<signal name="QUAD-A">
<contactref element="SW2" pad="A"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="QUAD-C">
<contactref element="J1" pad="7"/>
<contactref element="SW2" pad="C"/>
</signal>
<signal name="QUAD-B">
<contactref element="SW2" pad="B"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="PUSHBUTTON">
<contactref element="J1" pad="5"/>
<contactref element="SW2" pad="3"/>
</signal>
<signal name="BLUE">
<contactref element="R3" pad="P$1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="GREEN">
<contactref element="R2" pad="P$1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RED">
<contactref element="R1" pad="P$1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="LED-SWITCH-COM">
<contactref element="SW2" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="SW2" pad="4"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="P$2"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="SW2" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
