<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<hole x="-25" y="57" drill="3.2"/>
<hole x="25" y="57" drill="3.2"/>
<text>UP</text>
<text>C64 Expansionsport Adapter</text>
</plain>
<libraries>
<library name="0RB_Commodore">
<packages>
<package name="EXPANSIONPORT">
</package>
</packages>
</library>
<library name="C64 Expansionsport">
<packages>
<package name="CARTRIDGE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="C64 Expansionsport" package="CARTRIDGE" value="Port"/>
<element name="CN1" library="0RB_Commodore" package="EXPANSIONPORT" value="EXPANSIONPORT-C64"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="21"/>
<contactref element="CN1" pad="21"/>
</signal>
<signal name="N$2">
<contactref element="CN1" pad="20"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="19"/>
<contactref element="CN1" pad="19"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="18"/>
<contactref element="CN1" pad="18"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="17"/>
<contactref element="CN1" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="16"/>
<contactref element="CN1" pad="16"/>
</signal>
<signal name="N$7">
<contactref element="CN1" pad="15"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="14"/>
<contactref element="CN1" pad="14"/>
</signal>
<signal name="N$14">
<contactref element="CN1" pad="M"/>
<contactref element="U$1" pad="M"/>
</signal>
<signal name="N$15">
<contactref element="CN1" pad="N"/>
<contactref element="U$1" pad="N"/>
</signal>
<signal name="N$16">
<contactref element="CN1" pad="P"/>
<contactref element="U$1" pad="P"/>
</signal>
<signal name="N$17">
<contactref element="CN1" pad="R"/>
<contactref element="U$1" pad="R"/>
</signal>
<signal name="N$18">
<contactref element="CN1" pad="S"/>
<contactref element="U$1" pad="S"/>
</signal>
<signal name="N$19">
<contactref element="CN1" pad="T"/>
<contactref element="U$1" pad="T"/>
</signal>
<signal name="N$20">
<contactref element="CN1" pad="U"/>
<contactref element="U$1" pad="U"/>
</signal>
<signal name="N$21">
<contactref element="CN1" pad="V"/>
<contactref element="U$1" pad="V"/>
</signal>
<signal name="N$22">
<contactref element="CN1" pad="W"/>
<contactref element="U$1" pad="W"/>
</signal>
<signal name="N$23">
<contactref element="CN1" pad="X"/>
<contactref element="U$1" pad="X"/>
</signal>
<signal name="N$24">
<contactref element="CN1" pad="Y"/>
<contactref element="U$1" pad="Y"/>
</signal>
<signal name="N$9">
<contactref element="CN1" pad="L"/>
<contactref element="U$1" pad="L"/>
</signal>
<signal name="N$10">
<contactref element="CN1" pad="K"/>
<contactref element="U$1" pad="K"/>
</signal>
<signal name="N$11">
<contactref element="CN1" pad="J"/>
<contactref element="U$1" pad="J"/>
</signal>
<signal name="N$12">
<contactref element="CN1" pad="H"/>
<contactref element="U$1" pad="H"/>
</signal>
<signal name="N$13">
<contactref element="CN1" pad="F"/>
<contactref element="U$1" pad="F"/>
</signal>
<signal name="N$27">
<contactref element="CN1" pad="22"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="N$29">
<contactref element="CN1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="B"/>
<contactref element="CN1" pad="B"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="C"/>
<contactref element="CN1" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="D"/>
<contactref element="CN1" pad="D"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="E"/>
<contactref element="CN1" pad="E"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="A"/>
<contactref element="CN1" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="CN1" pad="Z"/>
<contactref element="U$1" pad="Z"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="2"/>
<contactref element="CN1" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="3"/>
<contactref element="CN1" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="4"/>
<contactref element="CN1" pad="4"/>
</signal>
<signal name="N$37">
<contactref element="U$1" pad="5"/>
<contactref element="CN1" pad="5"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="6"/>
<contactref element="CN1" pad="6"/>
</signal>
<signal name="N$39">
<contactref element="U$1" pad="7"/>
<contactref element="CN1" pad="7"/>
</signal>
<signal name="N$40">
<contactref element="U$1" pad="8"/>
<contactref element="CN1" pad="8"/>
</signal>
<signal name="N$41">
<contactref element="U$1" pad="9"/>
<contactref element="CN1" pad="9"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="10"/>
<contactref element="CN1" pad="10"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="11"/>
<contactref element="CN1" pad="11"/>
</signal>
<signal name="N$43">
<contactref element="U$1" pad="12"/>
<contactref element="CN1" pad="12"/>
</signal>
<signal name="N$44">
<contactref element="U$1" pad="13"/>
<contactref element="CN1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
