<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="36" y2="31" width="0" layer="20"/>
<wire x1="36" y1="31" x2="0" y2="31" width="0" layer="20"/>
<wire x1="0" y1="31" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>PWR IN</text>
<text>24V 12A</text>
<text>OUT</text>
<text>MAX</text>
</plain>
<libraries>
<library name="Cohesion_parts">
<packages>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="eric_sorensen">
<packages>
<package name="1715250000">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R35" library="resistor" package="R0603" value="10r">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="resistor" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="SML0603" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="resistor" package="R0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
<element name="D11" library="SparkFun-DiscreteSemi" package="SOD-323" value="1N4148">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="U$1" library="Cohesion_parts" package="D2PACK" value="MOSFET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="eric_sorensen" package="1715250000" value="5MMCONN"/>
<element name="U$2" library="eric_sorensen" package="1715250000" value="5MMCONN"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R36" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="FET-LOGIC-IN">
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="E1-CONTROL">
<contactref element="R37" pad="2"/>
<contactref element="D11" pad="A"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$28">
<contactref element="R35" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="HEATERVIN">
<contactref element="LED7" pad="A"/>
<contactref element="D11" pad="C"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="N$30">
<contactref element="R37" pad="1"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
