<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<description>Logic Level Converter
3.3V - 5V DC
Phantomic Labs, LLC</description>
<plain>
<wire x1="0" y1="0" x2="0" y2="25.4" width="0.254" layer="20"/>
<wire x1="0" y1="25.4" x2="17.78" y2="25.4" width="0.254" layer="20"/>
<wire x1="17.78" y1="25.4" x2="17.78" y2="0" width="0.254" layer="20"/>
<wire x1="17.78" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>GND</text>
<text>B8</text>
<text>B7</text>
<text>B6</text>
<text>B5</text>
<text>B4</text>
<text>B3</text>
<text>B2</text>
<text>5V</text>
<text>B1</text>
<text>OE</text>
<text>A8</text>
<text>A7</text>
<text>A6</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>3V3</text>
<text>A1</text>
<text>3.3V - 5V DC
Logic Level Converter
Phantomic Labs, LLC
</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="Ai_IC">
<description>&lt;h3&gt;Ai IC&lt;/h3&gt;
&lt;p&gt;
This library includes digital and analog Integrated Circuits such as MCUs, shift registers, etc. (Excludes power ICs such as regulators, and RF ICs such as Wi-Fi and Bluetooth)
&lt;/p&gt;</description>
<packages>
<package name="TSSOP20">
</package>
</packages>
</library>
<library name="dp_devices.v6">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="C805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Ai_IC" package="TSSOP20" value="TXB0108">
<attribute name="NAME"/>
</element>
<element name="C1" library="dp_devices.v6" package="C805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="dp_devices.v6" package="C805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="A1">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="A8">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="B8">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="B7">
<contactref element="U1" pad="13"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="B6">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="B5">
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="B4">
<contactref element="U1" pad="16"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="B3">
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="B2">
<contactref element="U1" pad="18"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="B1">
<contactref element="U1" pad="20"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="19"/>
<contactref element="J2" pad="9"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="OE">
<contactref element="U1" pad="10"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
