<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="8.89" x2="74.6" y2="8.89" width="0" layer="20"/>
<wire x1="74.6" y1="8.89" x2="74.6" y2="59.68" width="0" layer="20"/>
<wire x1="74.6" y1="59.68" x2="-1.27" y2="59.68" width="0" layer="20"/>
<wire x1="-1.27" y1="59.68" x2="-1.27" y2="8.89" width="0" layer="20"/>
<text>TRIG_OUT</text>
<text>Noise Audio Output</text>
<text>Song Audio Output</text>
<text>BNC 1</text>
<text>BNC 2</text>
<text>BNC 3</text>
</plain>
<libraries>
<library name="Teensy_Audioshield">
<packages>
<package name="AUDIOSHIELD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BNC">
<description>&lt;h3&gt;BNC Jack - Mouser Part#5227161 &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.mouser.com/ds/2/418/NG_CS_1307191_BNC_Connectors_0307-561881.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BNC&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="RHD2000_eval_board">
<description>Intan Technologies RHD2000 Eval Board</description>
<packages>
<package name="SJ-3523">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="Teensy_Audioshield" package="AUDIOSHIELD" value=""/>
<element name="TRIGGER_OUT" library="SparkFun-Connectors" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="LPA-12729"/>
<attribute name="SF_ID" value="PRT-10550"/>
<attribute name="VALUE"/>
</element>
<element name="AUDIO_OUTPUT" library="RHD2000_eval_board" package="SJ-3523" value="STEREO_JACK_SJ-3523">
<attribute name="NAME"/>
</element>
<element name="NOISE_OUTPUT" library="RHD2000_eval_board" package="SJ-3523" value="STEREO_JACK_SJ-3523">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$4">
<contactref element="TRIGGER_OUT" pad="S"/>
<contactref element="U$3" pad="9"/>
<contactref element="AUDIO_OUTPUT" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="AUDIO_OUTPUT" pad="2"/>
<contactref element="U$3" pad="OUTL"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="OUTR"/>
<contactref element="NOISE_OUTPUT" pad="3"/>
<contactref element="NOISE_OUTPUT" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="NOISE_OUTPUT" pad="1"/>
<contactref element="U$3" pad="OUTGND"/>
<contactref element="AUDIO_OUTPUT" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="GND"/>
<contactref element="TRIGGER_OUT" pad="GND"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
