<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="19.475" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="18.3" y2="0" width="0" layer="20"/>
<wire x1="18.3" y1="0" x2="20.3" y2="2" width="0" layer="20" curve="90"/>
<wire x1="20.3" y1="2" x2="20.3" y2="19.475" width="0" layer="20"/>
<wire x1="20.3" y1="19.475" x2="12.8" y2="26.975" width="0" layer="20" curve="90"/>
<wire x1="12.8" y1="26.975" x2="7.5" y2="26.975" width="0" layer="20"/>
<wire x1="7.5" y1="26.975" x2="0" y2="19.475" width="0" layer="20" curve="90"/>
<circle x="10.16" y="15.875" radius="4.016090625" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="allegro">
<description>&lt;b&gt;Allegro MicroSystems, Inc&lt;/b&gt;&lt;p&gt;
www.allegromicro.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIP3-UA">
<description>&lt;b&gt;Type: 3-pin SIP, conventional leadframe&lt;/b&gt;&lt;p&gt;
Source: http://www.allegromicro.com/en/Products/Packaging/pkghall1.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_2MM">
<description>&lt;h3&gt;Plated Through Hole - 2mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="0805" value=""/>
<element name="C2" library="SparkFun" package="0805" value=""/>
<element name="IC1" library="allegro" package="SIP3-UA" value="A1202UA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="IC2" library="allegro" package="SIP3-UA" value="A1202UA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_LOCK_LONGPADS" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="R1" library="SparkFun" package="0603-RES" value=""/>
<element name="R2" library="SparkFun" package="0603-RES" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="+V">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
