<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="24.13" x2="0" y2="1.905" width="0" layer="20"/>
<wire x1="0" y1="1.905" x2="1.905" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.905" y1="0" x2="3.81739375" y2="0" width="0" layer="20"/>
<wire x1="3.81739375" y1="0" x2="4.94970625" y2="0.37304375" width="0" layer="20" curve="36.469162"/>
<wire x1="4.94970625" y1="0.37304375" x2="18.277315625" y2="10.223884375" width="0" layer="20"/>
<wire x1="18.277315625" y1="10.223884375" x2="19.05" y2="11.755840625" width="0" layer="20" curve="53.530762"/>
<wire x1="19.05" y1="11.755840625" x2="19.05" y2="24.13" width="0" layer="20"/>
<wire x1="19.05" y1="24.13" x2="17.78" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="25.4" x2="1.27" y2="25.4" width="0" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0" layer="20" curve="90"/>
<text>+5VDC</text>
<text>GND</text>
<text>+5VDC</text>
<text>D2_DATA</text>
<text>D3_CLK</text>
<text>GND</text>
<text>GND</text>
<text>D2_DATA</text>
<text>D3_CLK</text>
<text>GND</text>
<text>VIN</text>
<text>PIXELPOWER_V0.1
TACTICAL SNACKS
20171202</text>
<text>ARDUINO NANO TO WS2801 LED
ADAPTER BOARD</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X03" value="NANO_LEFT_JPR"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="PIXEL"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="PWR"/>
<element name="JP5" library="SparkFun-Connectors" package="1X02" value="NANO_RIGHT_JPR"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP5" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="D2_DATA">
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="D3_CLK">
<contactref element="JP1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
