<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.9275" y2="0" width="0" layer="20"/>
<wire x1="54.9275" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<wire x1="54.9275" y1="25.4" x2="54.9275" y2="0" width="0" layer="20"/>
<text>C</text>
<text>L</text>
<text>H</text>
<text>Rev 1.10</text>
<text>1</text>
<text>2</text>
<text>+5</text>
<text>+5</text>
<text>15</text>
<text>GND</text>
<text>GND</text>
<text>16</text>
<text>3</text>
<text>5</text>
<text>7</text>
<text>9</text>
<text>11</text>
<text>13</text>
<text>4</text>
<text>6</text>
<text>8</text>
<text>10</text>
<text>12</text>
<text>14</text>
<text>CC-BY-SA 4.0</text>
<text>I2C RELAY/GPIO</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="RJ45-8">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="PJS">
<packages>
<package name="SOIC24">
</package>
<package name="3.2-MOUNT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value="AD0">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value="AD1">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="AD2">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="JP5" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="2X10" value="Relay Control/GPIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="PJS" package="SOIC24" value="PCA9671D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="MT1" library="PJS" package="3.2-MOUNT" value="3.2-MOUNT"/>
<element name="JP8" library="SparkFun-Connectors" package="1X02" value="HDR PWR">
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X02" value="BUS PWR">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="A2">
<contactref element="JP5" pad="5"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="A3">
<contactref element="JP5" pad="6"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="RL1">
<contactref element="IC1" pad="4"/>
<contactref element="JP4" pad="17"/>
</signal>
<signal name="RL2">
<contactref element="IC1" pad="5"/>
<contactref element="JP4" pad="18"/>
</signal>
<signal name="RL3">
<contactref element="IC1" pad="6"/>
<contactref element="JP4" pad="15"/>
</signal>
<signal name="RL4">
<contactref element="IC1" pad="7"/>
<contactref element="JP4" pad="16"/>
</signal>
<signal name="RL5">
<contactref element="IC1" pad="8"/>
<contactref element="JP4" pad="13"/>
</signal>
<signal name="RL6">
<contactref element="IC1" pad="9"/>
<contactref element="JP4" pad="14"/>
</signal>
<signal name="RL7">
<contactref element="IC1" pad="10"/>
<contactref element="JP4" pad="11"/>
</signal>
<signal name="RL8">
<contactref element="IC1" pad="11"/>
<contactref element="JP4" pad="12"/>
</signal>
<signal name="RL9">
<contactref element="IC1" pad="13"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="RL10">
<contactref element="IC1" pad="14"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="RL11">
<contactref element="IC1" pad="15"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="RL12">
<contactref element="IC1" pad="16"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="RL13">
<contactref element="IC1" pad="17"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="RL14">
<contactref element="IC1" pad="18"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="RL15">
<contactref element="IC1" pad="19"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="RL16">
<contactref element="IC1" pad="20"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="N$11">
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="JP3" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="A1">
<contactref element="JP5" pad="4"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="A0">
<contactref element="JP5" pad="3"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="A4-SDA">
<contactref element="JP5" pad="7"/>
<contactref element="JP6" pad="7"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="A5-SCL">
<contactref element="JP5" pad="8"/>
<contactref element="JP6" pad="8"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="BUSS_VCC">
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="JP9" pad="2"/>
<contactref element="JP8" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="24"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP4" pad="19"/>
<contactref element="JP4" pad="20"/>
<contactref element="JP8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
