<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="91.4275" y2="0" width="0" layer="20"/>
<wire x1="91.4275" y1="0" x2="91.4275" y2="50.79" width="0" layer="20"/>
<wire x1="91.4275" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.175" y="47.625" drill="3.2"/>
<hole x="3.175" y="3.175" drill="3.2"/>
<hole x="88.265" y="3.175" drill="3.2"/>
<hole x="88.265" y="47.625" drill="3.2"/>
<text>Wunder Weather Station</text>
<text>RV-BUILDERS PRODUCTS 2013</text>
<text>1</text>
<text>1</text>
<text>J6</text>
<text>1</text>
<text>Baro-Temp-Hyg</text>
<text>WiFi</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>NOT Ethernet !</text>
<text>PCB Revision B.2</text>
</plain>
<libraries>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wifi_WX">
<packages>
<package name="RJ45_VERT">
</package>
<package name="TQFP80-12X12">
<description>&lt;b&gt;TQFP80&lt;/b&gt; 12x12x1 mm Body&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
</package>
<package name="QFN24_4X4">
</package>
<package name="2X5FEMALE">
</package>
<package name="32005-301">
<description>&lt;b&gt;MINI USB-B R/A SMT W/O REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-301.pdf</description>
</package>
<package name="1X06_PIKIT">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X3_MOLEX_KK">
<description>Molex KK series pin header with frictiuon lock</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
<package name="TP10R">
</package>
<package name="TP06R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="CRYSTAL32_SMT">
</package>
<package name="1X02">
</package>
<package name="1X05">
</package>
<package name="RJ11-6-VERT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="wifi_WX" package="DPACK" value="3.3v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="22p">
<attribute name="NAME"/>
</element>
<element name="C14" library="rcl" package="C0603" value="22p">
<attribute name="NAME"/>
</element>
<element name="C1" library="rcl" package="SMC_B" value="22u/10v">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="SMC_D" value="330uF/6V">
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="rcl" package="R0603" value="8.2k">
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0603" value="26.1K">
<attribute name="NAME"/>
</element>
<element name="C9" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R13" library="rcl" package="R0603" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="C10" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="R8" library="rcl" package="R0603" value="14k">
<attribute name="NAME"/>
</element>
<element name="R10" library="rcl" package="R0603" value="26.1K">
<attribute name="NAME"/>
</element>
<element name="R4" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R15" library="rcl" package="R0603" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="C13" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R11" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="U2" library="microchip" package="SO-08" value="25LC512">
<attribute name="OC_NEWARK" value="96K4092"/>
<attribute name="MPN" value="25LC080/SN"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1137302"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="led" package="CHIP-LED0603" value="grn">
<attribute name="NAME"/>
</element>
<element name="L2" library="led" package="CHIP-LED0603" value="ambr">
<attribute name="NAME"/>
</element>
<element name="L3" library="led" package="CHIP-LED0603" value="red">
<attribute name="NAME"/>
</element>
<element name="R16" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R17" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R18" library="rcl" package="R0603" value="470o">
<attribute name="NAME"/>
</element>
<element name="S2" library="wifi_WX" package="TACTILE_SWITCH_SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
</element>
<element name="S1" library="wifi_WX" package="TACTILE_SWITCH_SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="R0603" value="120o">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0603" value="120o">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="rcl" package="SMC_B" value="22uF/10V">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="SMB" value="B140">
<attribute name="NAME"/>
</element>
<element name="J1" library="wifi_WX" package="RJ45_VERT" value="RJ45-8VERT"/>
<element name="U3" library="wifi_WX" package="TQFP80-12X12" value="PIC24FJ128GA008">
<attribute name="OC_NEWARK" value="56K7339"/>
<attribute name="MPN" value="PIC24FJ128GA008-I/PT"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1146521"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="wifi_WX" package="QFN24_4X4" value="CP2104-GM">
<attribute name="NAME"/>
</element>
<element name="J6" library="wifi_WX" package="2X5FEMALE" value="M05X22X5FE">
<attribute name="NAME"/>
</element>
<element name="USB" library="wifi_WX" package="32005-301" value="MINI-USB-32005-301"/>
<element name="JPROG" library="wifi_WX" package="1X06_PIKIT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="UART1" library="wifi_WX" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C1" library="wifi_WX" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN" library="wifi_WX" package="1X3_MOLEX_KK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SUN" library="wifi_WX" package="1X3_MOLEX_KK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="wifi_WX" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
</element>
<element name="SV2" library="wifi_WX" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
</element>
<element name="SV3" library="wifi_WX" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
</element>
<element name="R12" library="rcl" package="R0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R14" library="rcl" package="R0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="RESET" library="wifi_WX" package="TACTILE_SWITCH_SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
</element>
<element name="R7" library="rcl" package="R0603" value="14k">
<attribute name="NAME"/>
</element>
<element name="R9" library="rcl" package="R0603" value="26.1K">
<attribute name="NAME"/>
</element>
<element name="R19" library="rcl" package="R0603" value="14k">
<attribute name="NAME"/>
</element>
<element name="R20" library="rcl" package="R0603" value="14k">
<attribute name="NAME"/>
</element>
<element name="R21" library="rcl" package="R0603" value="26.1K">
<attribute name="NAME"/>
</element>
<element name="R22" library="rcl" package="R0603" value="26.1K">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C20" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C21" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R23" library="rcl" package="R0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R24" library="rcl" package="R0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="TP1" library="wifi_WX" package="TP10R" value="TP10R">
<attribute name="NAME"/>
</element>
<element name="TP2" library="wifi_WX" package="TP06R" value="TP6R">
<attribute name="NAME"/>
</element>
<element name="TP3" library="wifi_WX" package="TP06R" value="TP6R">
<attribute name="NAME"/>
</element>
<element name="Q1" library="wifi_WX" package="CRYSTAL32_SMT" value="32.768Khz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RAIN" library="wifi_WX" package="1X02" value="M02">
<attribute name="NAME"/>
</element>
<element name="+5V" library="wifi_WX" package="1X3_MOLEX_KK" value="">
<attribute name="NAME"/>
</element>
<element name="ANA" library="wifi_WX" package="1X05" value=""/>
<element name="D2" library="diode" package="SOD123" value="MBR0520LT">
<attribute name="NAME"/>
</element>
<element name="J5" library="wifi_WX" package="RJ11-6-VERT" value="RJ11-6RJ11-VERT_LP"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="C15" pad="1"/>
<contactref element="U3" pad="59"/>
<contactref element="Q1" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="IC1" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="S2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C12" pad="-"/>
<contactref element="J1" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="U3" pad="51"/>
<contactref element="U3" pad="26"/>
<contactref element="U3" pad="31"/>
<contactref element="U3" pad="11"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="25"/>
<contactref element="J6" pad="2"/>
<contactref element="USB" pad="5_USB_GND"/>
<contactref element="JPROG" pad="3"/>
<contactref element="U3" pad="23"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="UART1" pad="2"/>
<contactref element="I2C1" pad="2"/>
<contactref element="USB" pad="M2"/>
<contactref element="USB" pad="M3"/>
<contactref element="USB" pad="M4"/>
<contactref element="USB" pad="M1"/>
<contactref element="SUN" pad="3"/>
<contactref element="FAN" pad="3"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV3" pad="10"/>
<contactref element="L1" pad="C"/>
<contactref element="L2" pad="C"/>
<contactref element="L3" pad="C"/>
<contactref element="RESET" pad="3"/>
<contactref element="S2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="RESET" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="RAIN" pad="1"/>
<contactref element="+5V" pad="3"/>
<contactref element="ANA" pad="1"/>
<contactref element="J5" pad="P$1"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="3"/>
<contactref element="C7" pad="+"/>
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="R15" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="12"/>
<contactref element="U3" pad="32"/>
<contactref element="U3" pad="48"/>
<contactref element="U3" pad="25"/>
<contactref element="U3" pad="71"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="J6" pad="10"/>
<contactref element="JPROG" pad="2"/>
<contactref element="SV1" pad="10"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="J5" pad="P$5"/>
</signal>
<signal name="MRF_RESET_">
<contactref element="U3" pad="55"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="MRF_SCK">
<contactref element="U3" pad="45"/>
<contactref element="J6" pad="8"/>
</signal>
<signal name="MRF_SDO">
<contactref element="U3" pad="44"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="MRF_SDI">
<contactref element="U3" pad="43"/>
<contactref element="J6" pad="9"/>
</signal>
<signal name="SCL1">
<contactref element="U3" pad="47"/>
<contactref element="R12" pad="2"/>
<contactref element="J5" pad="P$4"/>
</signal>
<signal name="SDA1">
<contactref element="U3" pad="46"/>
<contactref element="R14" pad="2"/>
<contactref element="J5" pad="P$3"/>
</signal>
<signal name="BARO_CS">
<contactref element="U3" pad="54"/>
<contactref element="J5" pad="P$2"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="21"/>
<contactref element="JPROG" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="22"/>
<contactref element="JPROG" pad="4"/>
</signal>
<signal name="MCU_RESET_">
<contactref element="U3" pad="9"/>
<contactref element="JPROG" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="P$3"/>
<contactref element="J1" pad="P$6"/>
<contactref element="SUN" pad="1"/>
<contactref element="FAN" pad="1"/>
<contactref element="+5V" pad="1"/>
<contactref element="ANA" pad="5"/>
</signal>
<signal name="USB_D-">
<contactref element="U1" pad="4"/>
<contactref element="USB" pad="2_D-"/>
</signal>
<signal name="USB_D+">
<contactref element="U1" pad="3"/>
<contactref element="USB" pad="3_D+"/>
</signal>
<signal name="WIND_ADC_IN">
<contactref element="R6" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="WIN_DIR_IN">
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="WIND_COUNT_IN">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="SUN_ADC_IN">
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U3" pad="17"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="SUN_IN">
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="P$5"/>
<contactref element="SUN" pad="2"/>
</signal>
<signal name="RAIN_COUNT">
<contactref element="R15" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C11" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="+"/>
<contactref element="U3" pad="70"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="N$27">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$32">
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$33">
<contactref element="U3" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U3" pad="3"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="SW_S2">
<contactref element="S2" pad="3"/>
<contactref element="U3" pad="38"/>
<contactref element="S2" pad="4"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="RAIN_CNT_IN">
<contactref element="J1" pad="P$7"/>
<contactref element="RAIN" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="WIND_COUNT">
<contactref element="R13" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="USB_TXD">
<contactref element="U3" pad="39"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="USB_RXD">
<contactref element="U3" pad="40"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="N$44">
<contactref element="U3" pad="41"/>
<contactref element="UART1" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="U3" pad="42"/>
<contactref element="UART1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C14" pad="1"/>
<contactref element="U3" pad="60"/>
<contactref element="Q1" pad="P$2"/>
</signal>
<signal name="N$47">
<contactref element="U3" pad="27"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="U3" pad="28"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="U3" pad="29"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="N$50">
<contactref element="U3" pad="30"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$51">
<contactref element="U3" pad="33"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$52">
<contactref element="U3" pad="34"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="N$53">
<contactref element="U3" pad="35"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="N$54">
<contactref element="U3" pad="36"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="N$66">
<contactref element="U3" pad="15"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="U3" pad="58"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="MRF_HIBER">
<contactref element="U3" pad="56"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="MRF_CS_">
<contactref element="U3" pad="57"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="8"/>
<contactref element="USB" pad="1_VBUS"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="61"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U3" pad="62"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U3" pad="63"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U3" pad="64"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="65"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="U3" pad="66"/>
<contactref element="SV2" pad="7"/>
</signal>
<signal name="N$35">
<contactref element="U3" pad="67"/>
<contactref element="SV2" pad="8"/>
</signal>
<signal name="N$36">
<contactref element="U3" pad="68"/>
<contactref element="SV2" pad="9"/>
</signal>
<signal name="N$40">
<contactref element="U3" pad="69"/>
<contactref element="SV2" pad="10"/>
</signal>
<signal name="N$41">
<contactref element="U3" pad="72"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="U3" pad="73"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="U3" pad="74"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="N$57">
<contactref element="U3" pad="75"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="N$58">
<contactref element="U3" pad="76"/>
<contactref element="SV3" pad="5"/>
</signal>
<signal name="N$59">
<contactref element="U3" pad="77"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="N$60">
<contactref element="U3" pad="78"/>
<contactref element="SV3" pad="7"/>
</signal>
<signal name="N$61">
<contactref element="U3" pad="79"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="N$62">
<contactref element="U3" pad="80"/>
<contactref element="SV3" pad="9"/>
</signal>
<signal name="N$63">
<contactref element="U3" pad="24"/>
<contactref element="JPROG" pad="6"/>
</signal>
<signal name="SCL2">
<contactref element="U3" pad="52"/>
<contactref element="I2C1" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="SDA2">
<contactref element="U3" pad="53"/>
<contactref element="I2C1" pad="3"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="WIFI_INT_">
<contactref element="U3" pad="13"/>
<contactref element="J6" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="49"/>
<contactref element="TP3" pad="TP_1"/>
</signal>
<signal name="N$5">
<contactref element="U3" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R16" pad="2"/>
<contactref element="L3" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="R17" pad="2"/>
<contactref element="L2" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="R18" pad="2"/>
<contactref element="L1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U3" pad="50"/>
<contactref element="TP2" pad="TP_1"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="14"/>
<contactref element="TP1" pad="TP_1"/>
</signal>
<signal name="N$22">
<contactref element="R9" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U3" pad="20"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R19" pad="2"/>
<contactref element="U3" pad="19"/>
<contactref element="R21" pad="2"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R20" pad="2"/>
<contactref element="U3" pad="18"/>
<contactref element="R22" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R20" pad="1"/>
<contactref element="ANA" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="R19" pad="1"/>
<contactref element="ANA" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="R7" pad="1"/>
<contactref element="ANA" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="SW_S1">
<contactref element="U3" pad="37"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="U1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
