<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="64.77" y1="2.54" x2="64.77" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="38.1" x2="0" y2="2.54" width="0" layer="20"/>
<text>12V</text>
<text>GND</text>
<text>PROX</text>
<text>DOSE</text>
<text>GND</text>
<text>5V</text>
<wire x1="64.77" y1="2.54" x2="62.23" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="64.77" y1="38.1" x2="62.23" y2="40.64" width="0" layer="20" curve="90"/>
<wire x1="0" y1="38.1" x2="2.54" y2="40.64" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="62.23" y2="0" width="0" layer="20"/>
<wire x1="2.54" y1="40.64" x2="62.23" y2="40.64" width="0" layer="20"/>
<text>PLUSMAZE_ARDUINO
2019 JULY 16
KIMTH@STANFORD.EDU</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>LICK</text>
</plain>
<libraries>
<library name="kimth">
<packages>
<package name="POLOLU_MAX14870">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="kimth" package="POLOLU_MAX14870" value="POLOLU_MAX14870"/>
<element name="U$2" library="kimth" package="POLOLU_MAX14870" value="POLOLU_MAX14870"/>
<element name="U$3" library="kimth" package="POLOLU_MAX14870" value="POLOLU_MAX14870"/>
<element name="U$4" library="kimth" package="POLOLU_MAX14870" value="POLOLU_MAX14870"/>
<element name="J1" library="SparkFun-Connectors" package="2X5" value="">
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="JP1" library="pinhead" package="1X03" value=""/>
<element name="JP2" library="pinhead" package="1X03" value=""/>
<element name="JP3" library="pinhead" package="1X03" value=""/>
<element name="JP4" library="pinhead" package="1X03" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="JP5" library="pinhead" package="1X03" value=""/>
<element name="JP6" library="pinhead" package="1X03" value=""/>
<element name="JP7" library="pinhead" package="1X03" value=""/>
<element name="JP8" library="pinhead" package="1X03" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="DGND">
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="9"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="U$4" pad="P$6"/>
<contactref element="U$3" pad="P$6"/>
<contactref element="U$4" pad="P$7"/>
<contactref element="U$4" pad="P$9"/>
<contactref element="U$3" pad="P$9"/>
<contactref element="U$3" pad="P$7"/>
<contactref element="U$1" pad="P$7"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="U$2" pad="P$9"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="DOSE4">
<contactref element="J1" pad="8"/>
<contactref element="U$4" pad="P$10"/>
</signal>
<signal name="DOSE3">
<contactref element="J1" pad="6"/>
<contactref element="U$3" pad="P$10"/>
</signal>
<signal name="DOSE2">
<contactref element="U$2" pad="P$10"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="DOSE1">
<contactref element="U$1" pad="P$10"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="J2" pad="1"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="U$4" pad="P$5"/>
</signal>
<signal name="12V">
<contactref element="J2" pad="2"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="PROX1">
<contactref element="JP1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="PROX2">
<contactref element="JP2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="PROX3">
<contactref element="JP3" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="PROX4">
<contactref element="JP4" pad="3"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="LICK1">
<contactref element="J4" pad="1"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="LICK2">
<contactref element="J4" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="LICK3">
<contactref element="J4" pad="3"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="LICK4">
<contactref element="J4" pad="4"/>
<contactref element="JP8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
