<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="1.3" y1="12" x2="18.7" y2="12" width="0.1" layer="20"/>
<text>SCL</text>
<text>SDA</text>
<text>INT</text>
<text>VDD</text>
<text>GND</text>
<wire x1="18.7" y1="0" x2="1.3" y2="0" width="0.1" layer="20"/>
<wire x1="18.7" y1="12" x2="18.7" y2="0" width="0.1" layer="20"/>
<wire x1="1.3" y1="12" x2="1.3" y2="0" width="0.1" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-24-TESTING">
<description>This is the testing package I pulled from the MPU-6050 breakout board. This package is tested and works.</description>
</package>
</packages>
</library>
<library name="con-garry">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;a href="www.mpe-connector.de"&gt;Menufacturer&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="332-02">
<description>&lt;b&gt;2 Pin - 2mm Dual Row&lt;/b&gt;&lt;p&gt;
Source: www.mpe-connector.de / garry_shortform_2012.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="headers(2mm)">
<packages>
<package name="1X1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0402-CAP" value=".1 uF"/>
<element name="C2" library="SparkFun-Passives" package="0402-CAP" value=".1 uF"/>
<element name="C3" library="SparkFun-Passives" package="0402-CAP" value="2.2 nF"/>
<element name="U1" library="SparkFun-Sensors" package="QFN-24-TESTING" value="MPU-6000QFN-24"/>
<element name="X1" library="con-garry" package="332-02" value="332-02"/>
<element name="X2" library="con-garry" package="332-02" value="332-02"/>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="10k"/>
<element name="J1" library="headers(2mm)" package="1X1" value="1X1"/>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="U1" pad="20"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="11"/>
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C2" pad="2"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="VDD">
<contactref element="C2" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="24"/>
<contactref element="X2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="23"/>
<contactref element="X2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="8"/>
<contactref element="SJ1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
