<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="91.05" y1="-84" x2="91.05" y2="10.61875" width="0" layer="20"/>
<wire x1="91.05" y1="10.61875" x2="87.05" y2="14.61875" width="0" layer="20" curve="90"/>
<wire x1="87.05" y1="14.61875" x2="-12" y2="14.61875" width="0" layer="20"/>
<wire x1="-12" y1="14.61875" x2="-16" y2="10.61875" width="0" layer="20" curve="90"/>
<wire x1="-16" y1="10.61875" x2="-16" y2="-84" width="0" layer="20"/>
<wire x1="-16" y1="-84" x2="-12" y2="-88" width="0" layer="20" curve="90"/>
<wire x1="-12" y1="-88" x2="87.05" y2="-88" width="0" layer="20"/>
<wire x1="87.05" y1="-88" x2="91.05" y2="-84" width="0" layer="20" curve="90"/>
<text>Paddr r1</text>
<text>by ayan4m1</text>
<hole x="-11.1125" y="-83.34375" drill="3"/>
<hole x="85.725" y="-83.34375" drill="3"/>
<hole x="85.725" y="-22.225" drill="3"/>
<hole x="-11.1125" y="10.31875" drill="3"/>
</plain>
<libraries>
<library name="Keyboard">
<description>Keyboard Keyswitch PCB footprints for MX and Alps switches.</description>
<packages>
<package name="MXHSPCB-1U">
<description>Keyboard switch package!</description>
</package>
<package name="MXHSPCB-2U-ROTATED">
<description>Keyboard switch package!</description>
</package>
<package name="MXHSPCB-2U">
<description>Keyboard switch package!</description>
</package>
</packages>
</library>
<library name="Controller">
<description>Footprints used for the controller and other supporting hardware</description>
<packages>
<package name="DO-35">
</package>
</packages>
</library>
<library name="RP2040_KEE_BOAR_DRIVER">
<packages>
<package name="RP2040_KEE_BOAR_DRIVER">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="WS2812">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NUMLK" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DNUMLK" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="SLASH" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DSLASH" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="ASTERISK" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DASTERISK" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="DASH" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DDASH" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="HOME" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DHOME" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="UP" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DUP" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="PGUP" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DPGUP" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="PLUS" library="Keyboard" package="MXHSPCB-2U-ROTATED" value="KEYSWITCH-PLAIN-MXHSPCB-2U-ROTATED">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DPLUS" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="LEFT" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DLEFT" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="5" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D5" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="RIGHT" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DRIGHT" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="END" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DEND" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="DOWN" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DDOWN" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="PGDN" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DPGDN" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="ENTER" library="Keyboard" package="MXHSPCB-2U-ROTATED" value="KEYSWITCH-PLAIN-MXHSPCB-2U-ROTATED">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DENTER" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="INS" library="Keyboard" package="MXHSPCB-2U" value="KEYSWITCH-PLAIN-MXHSPCB-2U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DINS" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="DEL" library="Keyboard" package="MXHSPCB-1U" value="KEYSWITCH-PLAIN-MXHSPCB-1U">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="DDEL" library="Controller" package="DO-35" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="U2" library="RP2040_KEE_BOAR_DRIVER" package="RP2040_KEE_BOAR_DRIVER" value="RP2040_KEE_BOAR_DRIVER"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="LED1" library="WS2812" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="LED2" library="WS2812" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="LED3" library="WS2812" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="LED4" library="WS2812" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="DNUMLK" pad="A"/>
<contactref element="NUMLK" pad="MX2"/>
</signal>
<signal name="ROW1">
<contactref element="DSLASH" pad="C"/>
<contactref element="DNUMLK" pad="C"/>
<contactref element="DASTERISK" pad="C"/>
<contactref element="DDASH" pad="C"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="N$2">
<contactref element="DSLASH" pad="A"/>
<contactref element="SLASH" pad="MX2"/>
</signal>
<signal name="N$3">
<contactref element="DASTERISK" pad="A"/>
<contactref element="ASTERISK" pad="MX2"/>
</signal>
<signal name="N$4">
<contactref element="DDASH" pad="A"/>
<contactref element="DASH" pad="MX2"/>
</signal>
<signal name="COL1">
<contactref element="HOME" pad="MX1"/>
<contactref element="NUMLK" pad="MX1"/>
<contactref element="LEFT" pad="MX1"/>
<contactref element="END" pad="MX1"/>
<contactref element="INS" pad="MX1"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="N$5">
<contactref element="DHOME" pad="A"/>
<contactref element="HOME" pad="MX2"/>
</signal>
<signal name="ROW2">
<contactref element="DUP" pad="C"/>
<contactref element="DHOME" pad="C"/>
<contactref element="DPGUP" pad="C"/>
<contactref element="DPLUS" pad="C"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="COL2">
<contactref element="UP" pad="MX1"/>
<contactref element="SLASH" pad="MX1"/>
<contactref element="5" pad="MX1"/>
<contactref element="DOWN" pad="MX1"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="N$6">
<contactref element="DUP" pad="A"/>
<contactref element="UP" pad="MX2"/>
</signal>
<signal name="COL3">
<contactref element="PGUP" pad="MX1"/>
<contactref element="ASTERISK" pad="MX1"/>
<contactref element="RIGHT" pad="MX1"/>
<contactref element="PGDN" pad="MX1"/>
<contactref element="DEL" pad="MX1"/>
<contactref element="U2" pad="26"/>
</signal>
<signal name="N$7">
<contactref element="DPGUP" pad="A"/>
<contactref element="PGUP" pad="MX2"/>
</signal>
<signal name="COL4">
<contactref element="PLUS" pad="MX1"/>
<contactref element="DASH" pad="MX1"/>
<contactref element="ENTER" pad="MX1"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="N$8">
<contactref element="DPLUS" pad="A"/>
<contactref element="PLUS" pad="MX2"/>
</signal>
<signal name="N$9">
<contactref element="DLEFT" pad="A"/>
<contactref element="LEFT" pad="MX2"/>
</signal>
<signal name="ROW3">
<contactref element="D5" pad="C"/>
<contactref element="DLEFT" pad="C"/>
<contactref element="DRIGHT" pad="C"/>
<contactref element="U2" pad="21"/>
</signal>
<signal name="N$10">
<contactref element="D5" pad="A"/>
<contactref element="5" pad="MX2"/>
</signal>
<signal name="N$11">
<contactref element="DRIGHT" pad="A"/>
<contactref element="RIGHT" pad="MX2"/>
</signal>
<signal name="N$12">
<contactref element="DEND" pad="A"/>
<contactref element="END" pad="MX2"/>
</signal>
<signal name="ROW4">
<contactref element="DDOWN" pad="C"/>
<contactref element="DEND" pad="C"/>
<contactref element="DPGDN" pad="C"/>
<contactref element="DENTER" pad="C"/>
<contactref element="U2" pad="22"/>
</signal>
<signal name="N$13">
<contactref element="DDOWN" pad="A"/>
<contactref element="DOWN" pad="MX2"/>
</signal>
<signal name="N$14">
<contactref element="DPGDN" pad="A"/>
<contactref element="PGDN" pad="MX2"/>
</signal>
<signal name="N$15">
<contactref element="DENTER" pad="A"/>
<contactref element="ENTER" pad="MX2"/>
</signal>
<signal name="N$16">
<contactref element="DINS" pad="A"/>
<contactref element="INS" pad="MX2"/>
</signal>
<signal name="ROW5">
<contactref element="DDEL" pad="C"/>
<contactref element="DINS" pad="C"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="N$17">
<contactref element="DDEL" pad="A"/>
<contactref element="DEL" pad="MX2"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="LED1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="LED3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="LED4" pad="3"/>
<contactref element="LED3" pad="3"/>
<contactref element="LED2" pad="3"/>
</signal>
<signal name="LED">
<contactref element="U2" pad="12"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="LED3" pad="2"/>
<contactref element="LED4" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
