<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="42.5" x2="30.5" y2="42.5" width="0.1524" layer="20"/>
<wire x1="30.5" y1="42.5" x2="30.5" y2="80" width="0.1524" layer="20"/>
<wire x1="30.5" y1="80" x2="0" y2="80" width="0.1524" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="42.5" width="0.1524" layer="20"/>
<text>Capacitance Meter</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="_hhn_diodes_smd">
<description>&lt;b&gt;Diodes&lt;/b&gt;</description>
<packages>
<package name="MELF-MLL41_DO213AB">
<description>&lt;p&gt;&lt;b&gt;MELF-MLL41 = DO213AB&lt;/b&gt;&lt;br /&gt;
Package DO-213AB = http://www.diotec.com/pdf/sm4001.pdf&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="1X06_NO_SILK_YES_STOP">
</package>
<package name="1X02_POLAR">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OS">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>SparkFun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="jameslbr">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="DIL12">
</package>
<package name="TO-92-AMMO">
</package>
<package name="CRYSTAL-OSC-SMD-5X3.2-2PAD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10u"/>
<element name="C6" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100u"/>
<element name="C7" library="SparkFun-Passives" package="0805" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="_hhn_diodes_smd" package="MELF-MLL41_DO213AB" value="SM4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="2X3" value="ISCP">
<attribute name="PROD_ID" value="CONN-09701"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="CAP"/>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="CAP"/>
<element name="J1" library="SparkFun-Connectors" package="1X02_POLAR" value="6-18VDC"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0805" value="3.3M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="R15" library="SparkFun-Passives" package="0805" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Passives" package="0805" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0805" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="0805" value="120R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="OS" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="jameslbr" package="TQFP32-08" value="ATMEGA4820AU">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="jameslbr" package="DIL12" value="LED4-DIGITSMALL"/>
<element name="U1" library="jameslbr" package="TO-92-AMMO" value="LM78L05T92">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="jameslbr" package="CRYSTAL-OSC-SMD-5X3.2-2PAD" value="12MHZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R8" pad="1"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="1"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="1"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="ISP_SCK">
<contactref element="U$1" pad="17"/>
<contactref element="R13" pad="2"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R13" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="GND">
<contactref element="R16" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="6"/>
<contactref element="S2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="5V">
<contactref element="R15" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="ISP_MOSI">
<contactref element="U$1" pad="15"/>
<contactref element="R1" pad="2"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="14"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="10"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R7" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R8" pad="2"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="N$9">
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="28"/>
<contactref element="S2" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="27"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="23"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="24"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="25"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="26"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="20"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="ISP_NRST">
<contactref element="U$1" pad="29"/>
<contactref element="J8" pad="5"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="Y1" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="8"/>
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="5"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$30">
<contactref element="D1" pad="C"/>
<contactref element="C6" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="ISP_MISO">
<contactref element="J8" pad="1"/>
<contactref element="U$1" pad="16"/>
<contactref element="R12" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
