<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="81.27" x2="0" y2="72.39" width="0" layer="20"/>
<wire x1="0" y1="72.39" x2="39.37" y2="17.78" width="0" layer="20"/>
<wire x1="39.37" y1="17.78" x2="100.33" y2="17.78" width="0" layer="20"/>
<wire x1="100.33" y1="17.78" x2="100" y2="81.27" width="0" layer="20"/>
<wire x1="100" y1="81.27" x2="0" y2="81.27" width="0" layer="20"/>
<text>Adam Shai</text>
<text>December 2016</text>
<text>Random Dots Kinetogram Shield</text>
<text>close</text>
<text>center</text>
<text>far</text>
<text>NOSE POKES</text>
<text>NOSE POKES</text>
<text>WATER VALVES</text>
<text>WATER VALES</text>
<text>5V</text>
<text>GND</text>
<text>26</text>
<text>27</text>
<text>36</text>
<text>37</text>
<text>46</text>
<text>47</text>
<text>5</text>
<text>3</text>
<text>5V
GND
SIG
GND</text>
<text>5V
GND
SIG
GND</text>
<text>DI</text>
<text>DI</text>
<text>DI</text>
<text>LEFT SPEAKER</text>
<text>RIGHT SPEAKER</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h1&gt;DC Barrel Jack Adapter - Breadboard Compatible&lt;/h1&gt;
&lt;h2&gt;PRT-10811&lt;/h2&gt;</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14/8">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SOL1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="SOL2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="SOL3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="POKE1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="POKE2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="POKE3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ic-package" package="DIL14/8" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ic-package" package="DIL14/8" value="">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="ic-package" package="DIL14/8" value="">
<attribute name="VALUE"/>
</element>
<element name="12V_JACK" library="SparkFun-Connectors" package="POWER_JACK_PTH_BREAD" value="POWER_JACKPTH_BREAD">
<attribute name="PROD_ID" value="PRT-10811"/>
</element>
<element name="5V" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="pinhead" package="1X01" value=""/>
<element name="RIGHT" library="pinhead" package="1X01" value=""/>
<element name="LEFT" library="pinhead" package="1X01" value=""/>
<element name="CLOSE" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MIDDLE" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAR" library="pinhead" package="1X02" value=""/>
<element name="GND1" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="5V1" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="DIG50">
<contactref element="POKE3" pad="3"/>
<contactref element="FAR" pad="1"/>
</signal>
<signal name="DIG51">
<contactref element="IC3" pad="2"/>
<contactref element="FAR" pad="2"/>
</signal>
<signal name="DIG31">
<contactref element="IC1" pad="2"/>
<contactref element="CLOSE" pad="2"/>
</signal>
<signal name="DIG30">
<contactref element="POKE1" pad="3"/>
<contactref element="CLOSE" pad="1"/>
</signal>
<signal name="DIG41">
<contactref element="IC2" pad="2"/>
<contactref element="MIDDLE" pad="2"/>
</signal>
<signal name="DIG40">
<contactref element="POKE2" pad="3"/>
<contactref element="MIDDLE" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="1"/>
<contactref element="12V_JACK" pad="PWR"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SOL3" pad="1"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="7"/>
<contactref element="SOL1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC2" pad="7"/>
<contactref element="SOL2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="POKE3" pad="1"/>
<contactref element="POKE2" pad="1"/>
<contactref element="POKE1" pad="1"/>
<contactref element="5V" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC3" pad="6"/>
<contactref element="SOL3" pad="2"/>
<contactref element="12V_JACK" pad="GND"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC2" pad="6"/>
<contactref element="SOL2" pad="2"/>
<contactref element="SOL1" pad="2"/>
<contactref element="POKE2" pad="2"/>
<contactref element="POKE1" pad="2"/>
<contactref element="POKE3" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RIGHT" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LEFT" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="GND1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="5V1" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
