<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.4886" y2="0" width="0" layer="20"/>
<wire x1="48.4886" y1="0" x2="48.4886" y2="10.3378" width="0" layer="20"/>
<wire x1="48.4886" y1="10.3378" x2="28.0924" y2="10.3378" width="0" layer="20"/>
<wire x1="20.3962" y1="10.3378" x2="0" y2="10.3378" width="0" layer="20"/>
<wire x1="0" y1="10.3378" x2="0" y2="0" width="0" layer="20"/>
<wire x1="20.3962" y1="10.3378" x2="20.7518" y2="9.9822" width="0.002540625" layer="20"/>
<wire x1="20.7518" y1="9.9822" x2="27.7368" y2="9.9822" width="0.002540625" layer="20"/>
<wire x1="27.7368" y1="9.9822" x2="28.0924" y2="10.3378" width="0.002540625" layer="20"/>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-5050-IC">
<description>&lt;h3&gt;5060 SMD RGB LED&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Specifications:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.6mm&lt;/li&gt;
&lt;li&gt;Area: 5.0mm x 5.0mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/WS2812.pdf"&gt; WS2812&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Example device(s):&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;WS2812&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PAD1" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="S2" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="U1" library="SparkFun-LED" package="LED-TRICOLOR-5050-IC" value="WS2812">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11598"/>
</element>
<element name="U2" library="SparkFun-LED" package="LED-TRICOLOR-5050-IC" value="WS2812">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11598"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="5"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="PAD4" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="2" route="any" routetag="U1.DI"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="2" route="any" routetag="U1.DI"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="S1" pad="3"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="S2" pad="3"/>
<contactref element="PAD3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
