<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="7.62" y1="40.64" x2="72.39" y2="40.64" width="0.254" layer="20"/>
<wire x1="72.39" y1="40.64" x2="74.93" y2="38.1" width="0.254" layer="20" curve="-90"/>
<wire x1="74.93" y1="38.1" x2="74.93" y2="2.54" width="0.254" layer="20"/>
<wire x1="74.93" y1="2.54" x2="72.39" y2="0" width="0.254" layer="20" curve="-90"/>
<wire x1="72.39" y1="0" x2="7.62" y2="0" width="0.254" layer="20"/>
<wire x1="7.62" y1="0" x2="5.08" y2="2.54" width="0.254" layer="20" curve="-90"/>
<wire x1="5.08" y1="2.54" x2="5.08" y2="38.1" width="0.254" layer="20"/>
<wire x1="5.08" y1="38.1" x2="7.62" y2="40.64" width="0.254" layer="20" curve="-90"/>
<text>led0</text>
<text>led1</text>
<text>led2</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>3.3v</text>
<text>gnd</text>
<text>5v</text>
<text>gnd</text>
<text>5vdc</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>Symphonic
  Picnic</text>
<text>ShroomCity</text>
<text>NYU IDM</text>
<text>2016</text>
<text>PlayTimesSquared</text>
<text>PlayTimesSquared</text>
<text>PlayTimesSquared</text>
<text>PlayTimesSquared</text>
<text>200</text>
<text>200</text>
<text>200</text>
<text>3.3v
regulator</text>
<text>gnd</text>
<text>3.3v</text>
<text>5v</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>Teensy 3.2
+
Audio Adapter</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="SIMPLE_HOLE">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Teensy3.0">
<packages>
<package name="TEENSY_3.0_ALLANALOG-PGM">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="maxstream">
<description>&lt;b&gt;MaxSream&lt;/b&gt; XBee Products&lt;p&gt;
http://www.maxstream.net</description>
<packages>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="LED_LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BUTTON_0" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="BUTTON_1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="BUTTON_2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="0.1uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="4.7uF"/>
<element name="GND" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="SW1" library="special" package="EDG-04" value="">
<attribute name="VALUE"/>
</element>
<element name="TEENSY_3.0" library="Teensy3.0" package="TEENSY_3.0_ALLANALOG-PGM" value="TEENSY_3.0_ALLANALOGPINS-PGM"/>
<element name="U$1" library="SparkFun-PowerIC" package="78XXL" value="V_REG_LD1117VXX"/>
<element name="XB1" library="maxstream" package="XBEE-PRO" value="XBEE-PRO">
<attribute name="MF" value=""/>
<attribute name="MPN" value="XBP24-AWI-001"/>
<attribute name="OC_NEWARK" value="42M2667"/>
<attribute name="OC_FARNELL" value="1337916"/>
</element>
<element name="LED2" library="eagle-ltspice" package="LED_LD260" value="">
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="eagle-ltspice" package="LED_LD260" value="">
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="LED0" library="eagle-ltspice" package="LED_LD260" value="">
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R0" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R1" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R2" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="POWER_JACKPTH_LOCK">
<attribute name="PROD_ID" value="CONN-08197"/>
<attribute name="SF_ID" value="PRT-00119"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="H2" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="TEENSY_3.0" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY_3.0" pad="VBAT"/>
</signal>
<signal name="AREF">
<contactref element="TEENSY_3.0" pad="AREF"/>
</signal>
<signal name="VUSB">
<contactref element="TEENSY_3.0" pad="VUSB"/>
</signal>
<signal name="GND">
<contactref element="TEENSY_3.0" pad="GND"/>
<contactref element="TEENSY_3.0" pad="GND1"/>
<contactref element="TEENSY_3.0" pad="GND2"/>
<contactref element="XB1" pad="10"/>
<contactref element="GND" pad="P$1"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H4" pad="P$1"/>
<contactref element="H1" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="BUTTON_0" pad="1"/>
<contactref element="BUTTON_1" pad="1"/>
<contactref element="BUTTON_2" pad="1"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="8"/>
<contactref element="SW1" pad="7"/>
<contactref element="SW1" pad="6"/>
<contactref element="U$1" pad="IN"/>
<contactref element="R2" pad="1"/>
<contactref element="R0" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="H2" pad="P$1"/>
</signal>
<signal name="5VDC">
<contactref element="TEENSY_3.0" pad="VIN"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="OUT"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="XBEE_OUT">
<contactref element="XB1" pad="2"/>
<contactref element="TEENSY_3.0" pad="0"/>
</signal>
<signal name="3.3VDC">
<contactref element="XB1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="T3.3">
<contactref element="TEENSY_3.0" pad="3.3V"/>
<contactref element="TEENSY_3.0" pad="3.3V1"/>
<contactref element="TEENSY_3.0" pad="3.3V2"/>
</signal>
<signal name="MEMCS">
<contactref element="TEENSY_3.0" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="TEENSY_3.0" pad="7"/>
</signal>
<signal name="BCLK">
<contactref element="TEENSY_3.0" pad="9"/>
</signal>
<signal name="SDCS">
<contactref element="TEENSY_3.0" pad="10"/>
</signal>
<signal name="MCLK">
<contactref element="TEENSY_3.0" pad="11"/>
</signal>
<signal name="MISO">
<contactref element="TEENSY_3.0" pad="12"/>
</signal>
<signal name="XBEE_IN">
<contactref element="TEENSY_3.0" pad="1"/>
<contactref element="XB1" pad="3"/>
</signal>
<signal name="BUTTON_0">
<contactref element="TEENSY_3.0" pad="2"/>
<contactref element="BUTTON_0" pad="2"/>
</signal>
<signal name="BUTTON_1">
<contactref element="TEENSY_3.0" pad="3"/>
<contactref element="BUTTON_1" pad="2"/>
</signal>
<signal name="BUTTON_2">
<contactref element="TEENSY_3.0" pad="4"/>
<contactref element="BUTTON_2" pad="2"/>
</signal>
<signal name="SELECT_A">
<contactref element="SW1" pad="1"/>
<contactref element="TEENSY_3.0" pad="A10"/>
</signal>
<signal name="N$1">
<contactref element="TEENSY_3.0" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="TEENSY_3.0" pad="14/A0"/>
</signal>
<signal name="N$3">
<contactref element="TEENSY_3.0" pad="15/A1"/>
</signal>
<signal name="N$4">
<contactref element="TEENSY_3.0" pad="18/A4"/>
</signal>
<signal name="N$5">
<contactref element="TEENSY_3.0" pad="19/A5"/>
</signal>
<signal name="N$7">
<contactref element="TEENSY_3.0" pad="22/A8"/>
</signal>
<signal name="N$8">
<contactref element="TEENSY_3.0" pad="23/A9"/>
</signal>
<signal name="N$6">
<contactref element="TEENSY_3.0" pad="RST"/>
</signal>
<signal name="SELECT_C">
<contactref element="SW1" pad="3"/>
<contactref element="TEENSY_3.0" pad="21/A7"/>
</signal>
<signal name="SELECT_D">
<contactref element="SW1" pad="4"/>
<contactref element="TEENSY_3.0" pad="20/A6"/>
</signal>
<signal name="SELECT_B">
<contactref element="SW1" pad="2"/>
<contactref element="TEENSY_3.0" pad="A11"/>
</signal>
<signal name="N$9">
<contactref element="R0" pad="2"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="LED_1">
<contactref element="LED1" pad="A"/>
<contactref element="TEENSY_3.0" pad="17/A3"/>
</signal>
<signal name="N$11">
<contactref element="LED0" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LED_0">
<contactref element="LED0" pad="A"/>
<contactref element="TEENSY_3.0" pad="16/A2"/>
</signal>
<signal name="LED_2">
<contactref element="LED2" pad="A"/>
<contactref element="TEENSY_3.0" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
