<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="-0.1016" y1="0" x2="10.9728" y2="0" width="0" layer="20"/>
<wire x1="10.9728" y1="0" x2="10.9728" y2="7.5184" width="0" layer="20"/>
<wire x1="10.9728" y1="7.5184" x2="0.254" y2="7.5184" width="0" layer="20"/>
<wire x1="0.254" y1="7.5184" x2="0.254" y2="-0.0508" width="0" layer="20"/>
<wire x1="0.254" y1="-0.0508" x2="0.0508" y2="-0.0508" width="0" layer="20"/>
<text>p</text>
<text>n</text>
<text>in</text>
<text>3v</text>
<text>gnd</text>
<text>LVDS</text>
<text>xlator</text>
</plain>
<libraries>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-DBV">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; DBV (R-PDSO-G5)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps77001.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSW-103-02-S-S-RA">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST SOCKET&lt;/b&gt;&lt;p&gt;
Source: Samtec SSW.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$4" library="texas" package="SOT23-DBV" value="SN65LVDS1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="X3" library="con-samtec" package="SSW-103-02-S-S-RA" value="SSW-103-02-S-S-RA">
<attribute name="OC_NEWARK" value="11P9368"/>
<attribute name="MPN" value="SSW-103-02-S-S-RA"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-samtec" package="SSW-103-02-S-S-RA" value="SSW-103-02-S-S-RA">
<attribute name="OC_NEWARK" value="11P9368"/>
<attribute name="MPN" value="SSW-103-02-S-S-RA"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$5">
</signal>
<signal name="N$4">
</signal>
<signal name="N$10">
<contactref element="X3" pad="1"/>
<contactref element="U$4" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="X3" pad="2"/>
<contactref element="U$4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="X3" pad="3"/>
<contactref element="U$4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="4"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="3"/>
<contactref element="X4" pad="2"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
