<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="50.165" y1="33.02" x2="17.78" y2="33.02" width="0" layer="20"/>
<wire x1="17.78" y1="33.02" x2="15.24" y2="30.48" width="0" layer="20" curve="90"/>
<wire x1="15.24" y1="30.48" x2="15.24" y2="7.62" width="0" layer="20"/>
<wire x1="15.24" y1="7.62" x2="17.78" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="5.08" x2="50.165" y2="5.08" width="0" layer="20"/>
<wire x1="50.165" y1="5.08" x2="52.705" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="52.705" y1="7.62" x2="52.705" y2="30.48" width="0" layer="20"/>
<wire x1="52.705" y1="30.48" x2="50.165" y2="33.02" width="0" layer="20" curve="90"/>
<text>mpinner</text>
<text>v0</text>
<text>blinkie</text>
<text>on</text>
<text>ir</text>
<text>1</text>
<text>vcc</text>
<text>gnd</text>
<text>sck</text>
<text>miso</text>
<text>mosi</text>
<text>rst</text>
<text>5vdc </text>
<text>via 8bi8 crash 
[nsl] agwn</text>
<text>SpaceHippy [HRC]
of DisOrieNT</text>
</plain>
<libraries>
<library name="tpic">
<description>&lt;b&gt;TPIC Shift Registers with Power Outputs&lt;/b&gt;&lt;br&gt;
TPIC6[ABC]596&lt;br&gt;

Library will also work for the *595 parts. The *596 have an improved timing but are identical otherwise.&lt;br&gt;

Created by fchk@istda.com 05/2006&lt;br&gt;</description>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
<library name="NSL">
<description>&lt;b&gt;[Nullspace Library]&lt;/b&gt;&lt;p&gt;

Parts library for NULLSPACE Projects</description>
<packages>
<package name="AVR-6_SO20L$">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="NSL_BATTICON_20MM_CLIPPED">
</package>
<package name="1X06_EDGE">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="KPS-1290">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="mattsEagleParts">
<packages>
<package name="SEGMENT-HEADERS">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TSOP8523">
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="SIMPLE_HOLE_SM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="tpic" package="SO20W" value="TPIC6B596DW">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="NSL" package="AVR-6_SO20L$" value="AVR-6_TINY2313-*S*"/>
<element name="BAT1" library="NSL" package="NSL_BATTICON_20MM_CLIPPED" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Electromechanical" package="KPS-1290" value="SWITCH_SPDT">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="IC2" library="tpic" package="SO20W" value="TPIC6596DW">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="mattsEagleParts" package="SEGMENT-HEADERS" value=""/>
<element name="U$3" library="SparkFun-Sensors" package="TSOP8523" value="IRRECEIVERSMD">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="NSL" package="1X06_EDGE" value="1X06_PIN_HEADER"/>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE_SM" value="SEW_HOLE-SMALL"/>
<element name="H2" library="LilyPad-Wearables" package="SIMPLE_HOLE_SM" value="SEW_HOLE-SMALL"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE_SM" value="SEW_HOLE-SMALL"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE_SM" value="SEW_HOLE-SMALL"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="U$2" pad="S"/>
<contactref element="U$1" pad="20"/>
<contactref element="C2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="6"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="19"/>
<contactref element="BAT1" pad="2"/>
<contactref element="U$1" pad="10"/>
<contactref element="C2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="9"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$4" pad="5"/>
<contactref element="H1" pad="P$1"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H4" pad="P$1"/>
</signal>
<signal name="PGND">
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="R-PIN1">
<contactref element="LED1" pad="1"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$10">
<contactref element="LED1" pad="16"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="6"/>
<contactref element="LED1" pad="15"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="5"/>
<contactref element="LED1" pad="13"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="4"/>
<contactref element="LED1" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="LED1" pad="10"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="16"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="15"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="14"/>
<contactref element="LED1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="18"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="17"/>
<contactref element="IC1" pad="3"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="19"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="6"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="16"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="15"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="R-PIN5">
<contactref element="LED1" pad="8"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="R-PIN7">
<contactref element="LED1" pad="12"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="R-PIN6">
<contactref element="LED1" pad="9"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="R-PIN8">
<contactref element="LED1" pad="14"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="R-PIN2">
<contactref element="LED1" pad="2"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="R-PIN3">
<contactref element="LED1" pad="5"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="R-PIN4">
<contactref element="LED1" pad="7"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="18"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="BAT1" pad="1"/>
<contactref element="U$2" pad="P"/>
<contactref element="H2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
