<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="8.89" y1="0" x2="61.9" y2="0" width="0" layer="20"/>
<wire x1="61.9" y1="0" x2="61.9" y2="38.09" width="0" layer="20"/>
<wire x1="61.9" y1="38.09" x2="8.89" y2="38.09" width="0" layer="20"/>
<wire x1="8.89" y1="38.09" x2="8.89" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="commodore">
<description>A library which aims to include all commodore-related stuff. &lt;br&gt;&lt;br&gt;
See &lt;b&gt;http://github.com/spacerace/8bit-eagle-libs/&lt;/b&gt;</description>
<packages>
<package name="UPS24CONN">
</package>
</packages>
</library>
<library name="ESP12E_DEVKIT">
<packages>
<package name="ESP12E_DEVKIT">
<description>ESP12E_DEVKIT</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="USER-PORT" library="commodore" package="UPS24CONN" value="C64_USERPORT-CONN"/>
<element name="WIFI-MODULE" library="ESP12E_DEVKIT" package="ESP12E_DEVKIT" value="ESP12E_DEVKIT"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="USER-PORT" pad="N"/>
<contactref element="WIFI-MODULE" pad="GND@3"/>
</signal>
<signal name="N$2">
<contactref element="WIFI-MODULE" pad="TX"/>
<contactref element="USER-PORT" pad="B"/>
<contactref element="USER-PORT" pad="C"/>
<contactref element="USER-PORT" pad="7"/>
</signal>
<signal name="RX">
<contactref element="WIFI-MODULE" pad="RX"/>
<contactref element="USER-PORT" pad="M"/>
<contactref element="USER-PORT" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="WIFI-MODULE" pad="D2"/>
<contactref element="USER-PORT" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="USER-PORT" pad="D"/>
<contactref element="WIFI-MODULE" pad="D1"/>
</signal>
<signal name="N$7">
<contactref element="USER-PORT" pad="L"/>
<contactref element="USER-PORT" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="USER-PORT" pad="2"/>
<contactref element="WIFI-MODULE" pad="VIN"/>
</signal>
<signal name="RI">
<contactref element="WIFI-MODULE" pad="D8"/>
<contactref element="USER-PORT" pad="F"/>
</signal>
<signal name="DTR">
<contactref element="WIFI-MODULE" pad="D6"/>
<contactref element="USER-PORT" pad="E"/>
</signal>
<signal name="DCD">
<contactref element="WIFI-MODULE" pad="D4"/>
<contactref element="USER-PORT" pad="H"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
