<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="-0.254" x2="-0.254" y2="8.001" width="0.1524" layer="20"/>
<wire x1="-0.254" y1="8.001" x2="13.843" y2="8.001" width="0.1524" layer="20"/>
<wire x1="13.843" y1="8.001" x2="13.843" y2="-0.254" width="0.1524" layer="20"/>
<wire x1="13.843" y1="-0.254" x2="-0.254" y2="-0.254" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="0-dicons">
<description>&lt;b&gt;Silkscreen Icons, Legend Fields and Fiducials&lt;/b&gt;&lt;p&gt;
A collection of general purpose silkscreen icons, legends and label fields.
&lt;h4&gt;&lt;i&gt;Copyright (C) 2004, Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 01/08/2005&lt;/i&gt;&lt;/h4&gt;</description>
<packages>
<package name="ICON_MINUS">
<description>&lt;b&gt;ICON&lt;/b&gt;&lt;p&gt; Minus Symbol</description>
</package>
<package name="ICON_ARROW-T">
<description>&lt;b&gt;ICON&lt;/b&gt;&lt;p&gt; Arrow Tiny</description>
</package>
<package name="ICON_PLUS">
<description>&lt;b&gt;ICON&lt;/b&gt;&lt;p&gt; Plus Sign Symbol</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="0-adafruit">
<packages>
<package name="WS2812">
</package>
</packages>
</library>
<library name="WS2812">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Connectors" package="1X03_NO_SILK" value="INPUT"/>
<element name="JP11" library="SparkFun-Connectors" package="1X03_NO_SILK" value="OUTPUT"/>
<element name="E$1" library="0-dicons" package="ICON_MINUS" value=""/>
<element name="E$2" library="0-dicons" package="ICON_MINUS" value=""/>
<element name="E$4" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="E$5" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="LED1" library="0-adafruit" package="WS2812" value="WS2812"/>
<element name="LED2" library="WS2812" package="WS2812B" value="2812B">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="0-dicons" package="ICON_PLUS" value=""/>
<element name="U$2" library="0-dicons" package="ICON_PLUS" value=""/>
<element name="U$3" library="0-dicons" package="ICON_PLUS" value=""/>
<element name="U$4" library="0-dicons" package="ICON_PLUS" value=""/>
<element name="E$6" library="0-dicons" package="ICON_MINUS" value=""/>
<element name="E$7" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="E$8" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="E$9" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="E$3" library="0-dicons" package="ICON_MINUS" value=""/>
<element name="E$10" library="0-dicons" package="ICON_ARROW-T" value=""/>
<element name="E$11" library="0-dicons" package="ICON_ARROW-T" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="C1" pad="2"/>
<contactref element="JP10" pad="3"/>
<contactref element="JP11" pad="3"/>
<contactref element="LED1" pad="VDD"/>
<contactref element="LED1" pad="LEDVDD"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="LED1" pad="VSS"/>
<contactref element="LED1" pad="VSS"/>
<contactref element="LED2" pad="3"/>
</signal>
<signal name="DO">
<contactref element="JP11" pad="2"/>
<contactref element="LED1" pad="DO"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="DI">
<contactref element="JP10" pad="2"/>
<contactref element="LED1" pad="DI"/>
<contactref element="LED2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
