<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="92.69" y2="0" width="0" layer="20"/>
<wire x1="92.69" y1="0" x2="92.69" y2="58.09" width="0" layer="20"/>
<wire x1="92.69" y1="58.09" x2="0" y2="58.09" width="0" layer="20"/>
<wire x1="0" y1="58.09" x2="0" y2="0" width="0" layer="20"/>
<text>+-15 VDC IN</text>
<text>0-5 VDC OUT</text>
<text>5-7 VDC PWR</text>
<text>Level Shifter 002</text>
<text>02-12-2014</text>
</plain>
<libraries>
<library name="dc-dc-converter">
<description>&lt;b&gt;DC-DC Converters&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="NMA">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DBZ_R-PDSO-G3">
<description>&lt;b&gt;DBZ (R-PDSO-G3)&lt;/b&gt; SOT-23&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3223W">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Top Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MKDSN1,5/2-5,08">
<description>&lt;b&gt;MKDSN 1,5/ 2-5,08&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 13,5 A&lt;br&gt;
Nennspannung: 250 V&lt;br&gt;
Rastermaß: 5,08 mm&lt;br&gt;
Polzahl: 2&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Montage: Löten&lt;br&gt;
Anschlussrichtung Leiter/Platine: 0 °&lt;br&gt;
Artikelnummer: 1729128&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1729128.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DC1" library="dc-dc-converter" package="NMA" value="">
<attribute name="OC_NEWARK" value="61K3064"/>
<attribute name="MPN" value="NMA0515SC"/>
<attribute name="MF" value="C &amp; D TECHNOLOGIES, INC"/>
<attribute name="OC_FARNELL" value="1021434"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="SO14" value="AD8684R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun" package="SMB-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="1.67k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="1.67k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0805" value="1.67k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="0805" value="1.67k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0805" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="texas" package="DBZ_R-PDSO-G3" value="LM4041BIDBZ">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="texas" package="DBZ_R-PDSO-G3" value="LM4041BIDBZ">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OFFA" library="pot" package="3223W" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OFFB" library="pot" package="3223W" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun" package="0805" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GA" library="pot" package="3223W" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GB" library="pot" package="3223W" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INA" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
</element>
<element name="INB" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
</element>
<element name="OUTA" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUTB" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="con-phoenix-508" package="MKDSN1,5/2-5,08" value="MKDSN1,5/2-5,08">
<attribute name="OC_NEWARK" value="30M2397"/>
<attribute name="MPN" value="MKDSN 1,5/2-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792903"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="SOT23" value=""/>
<element name="D7" library="diode" package="SOT23" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="+15V">
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="DC1" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="-15V">
<contactref element="IC1" pad="11"/>
<contactref element="C1" pad="1"/>
<contactref element="DC1" pad="4"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="DC1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="INA" pad="1"/>
<contactref element="OUTA" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="INB" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="OFFB" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="OFFA" pad="1"/>
<contactref element="OUTB" pad="2"/>
<contactref element="D7" pad="1"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="1"/>
<contactref element="INA" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="OUTA" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="DC1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="PWR" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="DC1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="PWR" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="D2" pad="3"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="GA" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R9" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="OFFA" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="14"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="INB" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="3"/>
<contactref element="D4" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="OFFB" pad="2"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC4" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="OFFB" pad="3"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="9"/>
<contactref element="GB" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="OFFA" pad="2"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="GA" pad="2"/>
<contactref element="GA" pad="3"/>
<contactref element="IC1" pad="7"/>
<contactref element="R4" pad="2"/>
<contactref element="D6" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="GB" pad="3"/>
<contactref element="GB" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R8" pad="1"/>
<contactref element="OUTB" pad="1"/>
<contactref element="D7" pad="3"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$21">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
</signals>
</board>
</drawing>
</eagle>
