<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="1.6764" y1="0" x2="98.9076" y2="0" width="0" layer="20"/>
<wire x1="98.9076" y1="0" x2="98.9076" y2="51.9176" width="0" layer="20"/>
<wire x1="98.9076" y1="51.9176" x2="1.6764" y2="51.9176" width="0" layer="20"/>
<wire x1="1.6764" y1="51.9176" x2="1.6764" y2="0" width="0" layer="20"/>
<text>A0        A2</text>
<text>0</text>
<text>1</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>!INT</text>
<text>!RST</text>
<text>MOTORS:</text>
<text>T-SW</text>
<text>T-3V3</text>
<text>TCL</text>
<text>T-INT</text>
<text>T-DA</text>
<text>T-A-</text>
<text>T-A+</text>
<text>T-1V</text>
<text>T-PI</text>
<text>T-RD</text>
<text>REV 1.0</text>
<text>+5V</text>
<text>+12V</text>
<text>GND</text>
<text>GND</text>
<text>  1:Escalator Bounces
FAILURE: FAILURE: FAI
LURE: FAILURE: FAILUR
E: FAILURE: FAILURE:F
AILURE: FAILURE: FAIL
URE: FAILURE: FAILURE
: FAILURE: FAILURE: F
A</text>
</plain>
<libraries>
<library name="motor-driver">
<description>&lt;h3&gt;Toshiba stepper motor driver&lt;/h3&gt;
Contains a TB62212 symbol in an FNG (HTSSOP-48) housing</description>
<packages>
<package name="HTSSOP48DCA">
<description>&lt;b&gt;PowerPAD PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt;&lt;p&gt;
DCA (R-PDSO-G**)&lt;br&gt;
Source: http://focus.ti.com/lit/ml/mpds044/mpds044.pdf / slma002.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="connector">
<description>&lt;b&gt;GIC connector&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by bryan@kadzban.net&lt;/author&gt;</description>
<packages>
<package name="SHERLOCK-6">
<description>Molex Sherlock family 6-pin board connector</description>
</package>
<package name="GULL-WING">
<description>3x DIP switches</description>
</package>
<package name="RJ45-V-SHIELD*2">
<description>2x RJ-45 connectors, vertical orientation, shielded</description>
</package>
<package name="SWITCH">
<description>SPST pushbutton switch</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="C0508">
<description>&lt;b&gt;Ceramic Chip Capacitor 0306&lt;/b&gt;&lt;p&gt;
Metric Code Size 0816</description>
</package>
<package name="C0805">
<description>&lt;b&gt;Ceramic Chip Capacitor 0805&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C0306">
<description>&lt;b&gt;Ceramic Chip Capacitor 0306&lt;/b&gt;&lt;p&gt;
Metric Code Size 0816</description>
</package>
<package name="A0R-JMP">
<description>&lt;b&gt;0R Jumper&lt;/b&gt;&lt;p&gt;
chip 0603&lt;p&gt;
http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_04.pdf</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="L3X3MM">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="F1812">
<description>&lt;b&gt;0ZCG Series - PTC Resettable Fuses&lt;/b&gt;&lt;p&gt;
Source: http://www.belfuse.com/pdfs/0ZCG.pdf</description>
</package>
<package name="F0805">
<description>&lt;b&gt;0ZCK Series - PTC Resettable Fuses&lt;/b&gt;&lt;p&gt;
Source: http://www.belfuse.com/pdfs/0ZCK.pdf</description>
</package>
<package name="C-UCM-6MM">
<description>&lt;b&gt;UCM series electrolytic capacitor 6.3x7.7mm&lt;/b&gt;&lt;p&gt;
Source: 
http://nichicon-us.com/english/products/pdfs/e-ucm.pdf / http://products.nichicon.co.jp/en/pdf/XJA043/e-ch_ref.pdf</description>
</package>
<package name="C-UCM">
<description>&lt;b&gt;UCM series electrolytic capacitor 5x5.8mm&lt;/b&gt;&lt;p&gt;
Source: 
http://nichicon-us.com/english/products/pdfs/e-ucm.pdf / http://products.nichicon.co.jp/en/pdf/XJA043/e-ch_ref.pdf</description>
</package>
</packages>
</library>
<library name="i2c-driver">
<description>&lt;b&gt;I2C bus buffer and CAN transceiver&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by bryan@kadzban.net&lt;/author&gt;</description>
<packages>
<package name="TSSOP56-6">
<description>&lt;b&gt;TSSOP56&lt;/b&gt; Plastic thin shrink small outline package; 56 leads; body width 6.1mm AKA SOT364-1&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PCA9698.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSSOP16: plastic thin shrink small outline package; 16 leads; body width 4.4 mm&lt;/b&gt; SOT403-1&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PCA9616.pdf</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5566-4">
<description>&lt;b&gt;Mini FIT connector 4 pol&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="i2c-driver" package="TSSOP56-6" value="PCA9698">
<attribute name="MF" value="NXP"/>
<attribute name="MPN" value="PCA9698DGG"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="motor-driver" package="HTSSOP48DCA" value="TB62212FNG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="motor-driver" package="HTSSOP48DCA" value="TB62212FNG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="motor-driver" package="HTSSOP48DCA" value="TB62212FNG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C" library="connector" package="RJ45-V-SHIELD*2" value="RJ452-V"/>
<element name="R14" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R15" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R16" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R17" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R18" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R19" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R20" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R21" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R25" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R24" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R23" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R22" library="rcl" package="R1206" value="1">
<attribute name="NAME"/>
</element>
<element name="R8" library="rcl" package="R0805" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0603" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IO1" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO2" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO3" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO4" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO5" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO6" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO7" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO8" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO9" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO10" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO11" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="IO12" library="connector" package="SHERLOCK-6" value="6-1971800SH"/>
<element name="SW1" library="connector" package="GULL-WING" value="DIP-3-219"/>
<element name="R5" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="connector" package="SWITCH" value="SW-1825910-7">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="connector" package="SOT23" value="DMG2305UX">
<attribute name="NAME"/>
</element>
<element name="Q2" library="connector" package="SOT23" value="DMG2305UX">
<attribute name="NAME"/>
</element>
<element name="Q3" library="connector" package="SOT23" value="DMG2305UX">
<attribute name="NAME"/>
</element>
<element name="PWR" library="con-molex" package="5566-4" value="5566-4">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="connector" package="C0508" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="connector" package="C0508" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="connector" package="C0508" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="connector" package="C0306" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="i2c-driver" package="TSSOP16" value="PCA9616">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="connector" package="A0R-JMP" value="0R-JUMP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="connector" package="SOT23-5" value="PAM2305">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="connector" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="connector" package="L3X3MM" value="2.2 uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="connector" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="connector" package="F1812" value="1.5A">
<attribute name="NAME"/>
</element>
<element name="F2" library="connector" package="F0805" value="500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="connector" package="C-UCM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="connector" package="C-UCM-6MM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="connector" package="C0805" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U4" pad="12"/>
<contactref element="U4" pad="24"/>
<contactref element="U4" pad="37"/>
<contactref element="U4" pad="EXP"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="14"/>
<contactref element="U4" pad="35"/>
<contactref element="U4" pad="39"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="24"/>
<contactref element="U5" pad="37"/>
<contactref element="U5" pad="EXP"/>
<contactref element="U5" pad="10"/>
<contactref element="U5" pad="14"/>
<contactref element="U5" pad="35"/>
<contactref element="U5" pad="39"/>
<contactref element="U6" pad="12"/>
<contactref element="U6" pad="24"/>
<contactref element="U6" pad="37"/>
<contactref element="U6" pad="EXP"/>
<contactref element="U6" pad="10"/>
<contactref element="U6" pad="14"/>
<contactref element="U6" pad="35"/>
<contactref element="U6" pad="39"/>
<contactref element="U3" pad="51"/>
<contactref element="U3" pad="39"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="23"/>
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="6"/>
<contactref element="U4" pad="32"/>
<contactref element="U4" pad="31"/>
<contactref element="U5" pad="32"/>
<contactref element="U5" pad="31"/>
<contactref element="U6" pad="32"/>
<contactref element="U6" pad="31"/>
<contactref element="U6" pad="27"/>
<contactref element="U6" pad="28"/>
<contactref element="U5" pad="28"/>
<contactref element="U5" pad="27"/>
<contactref element="U4" pad="28"/>
<contactref element="U4" pad="27"/>
<contactref element="R10" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IO1" pad="3"/>
<contactref element="IO2" pad="3"/>
<contactref element="IO3" pad="3"/>
<contactref element="IO4" pad="3"/>
<contactref element="IO5" pad="3"/>
<contactref element="IO6" pad="3"/>
<contactref element="IO7" pad="3"/>
<contactref element="IO8" pad="3"/>
<contactref element="IO9" pad="3"/>
<contactref element="IO10" pad="3"/>
<contactref element="IO11" pad="3"/>
<contactref element="IO12" pad="3"/>
<contactref element="RST" pad="2"/>
<contactref element="PWR" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="RST" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U3" pad="30"/>
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="I2C" pad="5"/>
<contactref element="I2C" pad="13"/>
<contactref element="I2C" pad="S3"/>
<contactref element="I2C" pad="S4"/>
<contactref element="I2C" pad="S5"/>
<contactref element="I2C" pad="S6"/>
<contactref element="I2C" pad="S2"/>
<contactref element="I2C" pad="S1"/>
<contactref element="PWR" pad="3"/>
<contactref element="U4" pad="GND@1"/>
<contactref element="U4" pad="GND@4"/>
<contactref element="U4" pad="GND@2"/>
<contactref element="U4" pad="GND@3"/>
<contactref element="U5" pad="GND@1"/>
<contactref element="U5" pad="GND@4"/>
<contactref element="U5" pad="GND@2"/>
<contactref element="U5" pad="GND@3"/>
<contactref element="U6" pad="GND@1"/>
<contactref element="U6" pad="GND@4"/>
<contactref element="U6" pad="GND@2"/>
<contactref element="U6" pad="GND@3"/>
<contactref element="C16" pad="NEG"/>
<contactref element="C17" pad="NEG"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="U4" pad="25"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="U5" pad="25"/>
<contactref element="R21" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="U6" pad="25"/>
<contactref element="C9" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="C17" pad="POS"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="46"/>
<contactref element="R8" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SW1" pad="OUT3"/>
<contactref element="SW1" pad="OUT2"/>
<contactref element="SW1" pad="OUT1"/>
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RS_D1">
<contactref element="U4" pad="46"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="RS_C1">
<contactref element="U4" pad="26"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="RS_B1">
<contactref element="U4" pad="23"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="RS_A1">
<contactref element="U4" pad="3"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="RS_B3">
<contactref element="U6" pad="23"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="RS_C3">
<contactref element="U6" pad="26"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="RS_D3">
<contactref element="U6" pad="46"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="RS_A3">
<contactref element="U6" pad="3"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="IO0_0">
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="IO0_1">
<contactref element="U3" pad="4"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="IO0_2">
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="IO0_3">
<contactref element="U3" pad="7"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="IO0_4">
<contactref element="U3" pad="8"/>
<contactref element="U4" pad="44"/>
</signal>
<signal name="IO0_5">
<contactref element="U3" pad="9"/>
<contactref element="U4" pad="43"/>
</signal>
<signal name="IO0_6">
<contactref element="U3" pad="10"/>
<contactref element="U4" pad="42"/>
</signal>
<signal name="IO0_7">
<contactref element="U3" pad="12"/>
<contactref element="U4" pad="41"/>
</signal>
<signal name="IO1_0">
<contactref element="U3" pad="13"/>
<contactref element="IO3" pad="4"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="IO2_0">
<contactref element="U3" pad="22"/>
<contactref element="U5" pad="8"/>
</signal>
<signal name="IO1_1">
<contactref element="U3" pad="14"/>
<contactref element="IO4" pad="4"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="IO1_2">
<contactref element="U3" pad="15"/>
<contactref element="IO1" pad="4"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="IO1_3">
<contactref element="U3" pad="16"/>
<contactref element="IO2" pad="4"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="IO1_4">
<contactref element="U3" pad="17"/>
<contactref element="IO5" pad="4"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="IO1_5">
<contactref element="U3" pad="19"/>
<contactref element="IO6" pad="4"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="IO1_6">
<contactref element="U3" pad="20"/>
<contactref element="IO7" pad="4"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="IO1_7">
<contactref element="U3" pad="21"/>
<contactref element="IO8" pad="4"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="IO2_1">
<contactref element="U3" pad="24"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="IO2_2">
<contactref element="U3" pad="25"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="IO2_3">
<contactref element="U3" pad="26"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="IO2_4">
<contactref element="U3" pad="31"/>
<contactref element="U5" pad="44"/>
</signal>
<signal name="IO2_5">
<contactref element="U3" pad="32"/>
<contactref element="U5" pad="43"/>
</signal>
<signal name="IO2_6">
<contactref element="U3" pad="33"/>
<contactref element="U5" pad="42"/>
</signal>
<signal name="IO2_7">
<contactref element="U3" pad="35"/>
<contactref element="U5" pad="41"/>
</signal>
<signal name="RS_A2">
<contactref element="U5" pad="3"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="RS_B2">
<contactref element="U5" pad="23"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="RS_C2">
<contactref element="U5" pad="26"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="RS_D2">
<contactref element="U5" pad="46"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="+1V">
<contactref element="U5" pad="17"/>
<contactref element="U6" pad="17"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U4" pad="17"/>
<contactref element="U4" pad="18"/>
<contactref element="U4" pad="19"/>
<contactref element="U4" pad="21"/>
<contactref element="U5" pad="18"/>
<contactref element="U5" pad="19"/>
<contactref element="U5" pad="21"/>
<contactref element="U6" pad="18"/>
<contactref element="U6" pad="19"/>
<contactref element="U6" pad="21"/>
</signal>
<signal name="+1V1">
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="OSCM3">
<contactref element="U6" pad="48"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="OSCM2">
<contactref element="U5" pad="48"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="OSCM1">
<contactref element="U4" pad="48"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="OUT_A1-">
<contactref element="U4" pad="9"/>
<contactref element="IO1" pad="1"/>
</signal>
<signal name="OUT_A1+">
<contactref element="U4" pad="11"/>
<contactref element="IO1" pad="2"/>
</signal>
<signal name="OUT_B1-">
<contactref element="U4" pad="15"/>
<contactref element="IO2" pad="1"/>
</signal>
<signal name="OUT_B1+">
<contactref element="U4" pad="13"/>
<contactref element="IO2" pad="2"/>
</signal>
<signal name="OUT_C1-">
<contactref element="U4" pad="34"/>
<contactref element="IO3" pad="1"/>
</signal>
<signal name="OUT_C1+">
<contactref element="U4" pad="36"/>
<contactref element="IO3" pad="2"/>
</signal>
<signal name="OUT_D1-">
<contactref element="U4" pad="40"/>
<contactref element="IO4" pad="1"/>
</signal>
<signal name="OUT_D1+">
<contactref element="U4" pad="38"/>
<contactref element="IO4" pad="2"/>
</signal>
<signal name="OUT_A2-">
<contactref element="U5" pad="9"/>
<contactref element="IO5" pad="1"/>
</signal>
<signal name="OUT_A2+">
<contactref element="U5" pad="11"/>
<contactref element="IO5" pad="2"/>
</signal>
<signal name="OUT_A3-">
<contactref element="U6" pad="9"/>
<contactref element="IO9" pad="1"/>
</signal>
<signal name="OUT_B2-">
<contactref element="U5" pad="15"/>
<contactref element="IO6" pad="1"/>
</signal>
<signal name="OUT_B2+">
<contactref element="U5" pad="13"/>
<contactref element="IO6" pad="2"/>
</signal>
<signal name="OUT_C2-">
<contactref element="U5" pad="34"/>
<contactref element="IO7" pad="1"/>
</signal>
<signal name="OUT_C2+">
<contactref element="U5" pad="36"/>
<contactref element="IO7" pad="2"/>
</signal>
<signal name="OUT_D2-">
<contactref element="U5" pad="40"/>
<contactref element="IO8" pad="1"/>
</signal>
<signal name="OUT_D2+">
<contactref element="U5" pad="38"/>
<contactref element="IO8" pad="2"/>
</signal>
<signal name="OUT_A3+">
<contactref element="U6" pad="11"/>
<contactref element="IO9" pad="2"/>
</signal>
<signal name="OUT_B3-">
<contactref element="U6" pad="15"/>
<contactref element="IO10" pad="1"/>
</signal>
<signal name="OUT_B3+">
<contactref element="U6" pad="13"/>
<contactref element="IO10" pad="2"/>
</signal>
<signal name="OUT_C3-">
<contactref element="U6" pad="34"/>
<contactref element="IO11" pad="1"/>
</signal>
<signal name="OUT_C3+">
<contactref element="U6" pad="36"/>
<contactref element="IO11" pad="2"/>
</signal>
<signal name="OUT_D3-">
<contactref element="U6" pad="40"/>
<contactref element="IO12" pad="1"/>
</signal>
<signal name="OUT_D3+">
<contactref element="U6" pad="38"/>
<contactref element="IO12" pad="2"/>
</signal>
<signal name="IO4_3">
<contactref element="U3" pad="49"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="A2">
<contactref element="U3" pad="29"/>
<contactref element="R5" pad="2"/>
<contactref element="SW1" pad="IN1"/>
</signal>
<signal name="RST">
<contactref element="U3" pad="56"/>
<contactref element="RST" pad="4"/>
<contactref element="RST" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U3" pad="28"/>
<contactref element="SW1" pad="IN2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="IO4_5">
<contactref element="U3" pad="52"/>
<contactref element="U6" pad="43"/>
</signal>
<signal name="IO4_6">
<contactref element="U3" pad="53"/>
<contactref element="U6" pad="42"/>
</signal>
<signal name="IO4_7">
<contactref element="U3" pad="54"/>
<contactref element="U6" pad="41"/>
</signal>
<signal name="+5V_HF_1">
<contactref element="Q1" pad="3"/>
<contactref element="IO1" pad="5"/>
<contactref element="IO2" pad="5"/>
<contactref element="IO3" pad="5"/>
<contactref element="IO4" pad="5"/>
</signal>
<signal name="+5V_HF_3">
<contactref element="Q3" pad="3"/>
<contactref element="IO9" pad="5"/>
<contactref element="IO10" pad="5"/>
<contactref element="IO11" pad="5"/>
<contactref element="IO12" pad="5"/>
</signal>
<signal name="+5V_HF_2">
<contactref element="Q2" pad="3"/>
<contactref element="IO5" pad="5"/>
<contactref element="IO6" pad="5"/>
<contactref element="IO7" pad="5"/>
<contactref element="IO8" pad="5"/>
</signal>
<signal name="+5V">
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="16"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="I2C" pad="4"/>
<contactref element="I2C" pad="12"/>
<contactref element="C16" pad="POS"/>
</signal>
<signal name="INT">
<contactref element="U3" pad="55"/>
<contactref element="J1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="A0">
<contactref element="U3" pad="27"/>
<contactref element="R7" pad="2"/>
<contactref element="SW1" pad="IN3"/>
</signal>
<signal name="IO3_0">
<contactref element="U3" pad="36"/>
<contactref element="Q1" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="IO3_1">
<contactref element="U3" pad="37"/>
<contactref element="Q2" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="IO3_2">
<contactref element="U3" pad="38"/>
<contactref element="Q3" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="IO3_3">
<contactref element="U3" pad="40"/>
</signal>
<signal name="IO3_4">
<contactref element="U3" pad="41"/>
<contactref element="IO9" pad="4"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="IO3_5">
<contactref element="U3" pad="42"/>
<contactref element="IO10" pad="4"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="IO3_6">
<contactref element="U3" pad="43"/>
<contactref element="IO11" pad="4"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="IO3_7">
<contactref element="U3" pad="44"/>
<contactref element="IO12" pad="4"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="IO4_0">
<contactref element="U3" pad="45"/>
<contactref element="U6" pad="8"/>
</signal>
<signal name="IO4_1">
<contactref element="U3" pad="47"/>
<contactref element="U6" pad="7"/>
</signal>
<signal name="IO4_2">
<contactref element="U3" pad="48"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="INTRST">
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="SW">
<contactref element="U1" pad="5"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="DSDAM">
<contactref element="I2C" pad="1"/>
<contactref element="I2C" pad="9"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="DSDAP">
<contactref element="I2C" pad="2"/>
<contactref element="I2C" pad="10"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="DSCLM">
<contactref element="I2C" pad="6"/>
<contactref element="I2C" pad="14"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="DSCLP">
<contactref element="I2C" pad="3"/>
<contactref element="I2C" pad="11"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="DINTM">
<contactref element="U2" pad="11"/>
<contactref element="I2C" pad="7"/>
<contactref element="I2C" pad="15"/>
</signal>
<signal name="DINTP">
<contactref element="U2" pad="10"/>
<contactref element="I2C" pad="8"/>
<contactref element="I2C" pad="16"/>
</signal>
<signal name="+5V_ATX">
<contactref element="Q2" pad="2"/>
<contactref element="IO5" pad="6"/>
<contactref element="IO6" pad="6"/>
<contactref element="IO7" pad="6"/>
<contactref element="IO8" pad="6"/>
<contactref element="Q1" pad="2"/>
<contactref element="IO1" pad="6"/>
<contactref element="IO2" pad="6"/>
<contactref element="IO3" pad="6"/>
<contactref element="IO4" pad="6"/>
<contactref element="Q3" pad="2"/>
<contactref element="IO9" pad="6"/>
<contactref element="IO10" pad="6"/>
<contactref element="IO11" pad="6"/>
<contactref element="IO12" pad="6"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="F2" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="MODE2_1">
<contactref element="C7" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="30"/>
</signal>
<signal name="MODE2_2">
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="30"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="MODE2_3">
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="30"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="IO4_4">
<contactref element="U3" pad="50"/>
<contactref element="U6" pad="44"/>
</signal>
<signal name="ATX12V">
<contactref element="PWR" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="ATX5V">
<contactref element="PWR" pad="2"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="!PIDET">
<contactref element="U2" pad="5"/>
</signal>
<signal name="!READY">
<contactref element="U2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
