<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="22.9362" y1="10.5156" x2="75.2602" y2="10.5156" width="0" layer="20"/>
<wire x1="75.2602" y1="10.5156" x2="75.2602" y2="36.0426" width="0" layer="20"/>
<wire x1="75.2602" y1="36.0426" x2="22.9362" y2="36.0426" width="0" layer="20"/>
<wire x1="22.9362" y1="36.0426" x2="22.9362" y2="10.5156" width="0" layer="20"/>
<text>RELAY</text>
<text>START</text>
<text>ATMEGA328P-PU</text>
<text>REFLOW OVEN</text>
<text>CONTROL BOARD</text>
<text>THERMOCOUPLE</text>
<text>+</text>
<text>-</text>
<text>PWR</text>
</plain>
<libraries>
<library name="newStuff">
<packages>
<package name="LCM1602C">
</package>
<package name="MSOP8">
</package>
<package name="2PIN">
</package>
<package name="C0805">
</package>
<package name="RC0805">
</package>
<package name="EIA_TRIM">
</package>
<package name="SOT-23A-3">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QS">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="newStuff" package="LCM1602C" value="LCM1602C"/>
<element name="TCAMP" library="newStuff" package="MSOP8" value="AD8497ARMZ">
<attribute name="NAME"/>
</element>
<element name="TCIN" library="newStuff" package="2PIN" value="CONN2"/>
<element name="PWR" library="newStuff" package="2PIN" value="CONN2"/>
<element name="GO" library="newStuff" package="2PIN" value="CONN2"/>
<element name="RELAY" library="newStuff" package="2PIN" value="CONN2"/>
<element name="U1" library="SparkFun-DigitalIC" package="DIL28-3" value="ATMEGA328P_PDIP"/>
<element name="Q1" library="special" package="QS" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="newStuff" package="C0805" value="22p">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="newStuff" package="C0805" value="22p">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="newStuff" package="C0805" value="470n">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="newStuff" package="C0805" value="470n">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="newStuff" package="C0805" value="470n">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="newStuff" package="RC0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="U$8" library="newStuff" package="RC0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="U$9" library="newStuff" package="RC0805" value="1M">
<attribute name="VALUE"/>
</element>
<element name="U$11" library="newStuff" package="RC0805" value="100k">
<attribute name="VALUE"/>
</element>
<element name="U$12" library="newStuff" package="RC0805" value="LED">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="U$13" library="newStuff" package="EIA_TRIM" value="TRIMPOT"/>
<element name="U$10" library="newStuff" package="SOT-23A-3" value="VREG"/>
<element name="U$14" library="newStuff" package="C0805" value="1u">
<attribute name="VALUE"/>
</element>
<element name="U$15" library="newStuff" package="C0805" value="&lt;1u">
<attribute name="VALUE"/>
</element>
<element name="U$16" library="newStuff" package="C0805" value="1u">
<attribute name="VALUE"/>
</element>
<element name="U$17" library="newStuff" package="C0805" value="1u">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="9"/>
<contactref element="Q1" pad="2"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="10"/>
<contactref element="Q1" pad="1"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="PWR" pad="P$1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="U$11" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="RELAY" pad="P$2"/>
<contactref element="TCAMP" pad="P$7"/>
<contactref element="U$14" pad="P$1"/>
<contactref element="U$10" pad="TOP"/>
<contactref element="U$13" pad="P$1"/>
<contactref element="U$16" pad="P$1"/>
<contactref element="U$17" pad="P$1"/>
</signal>
<signal name="GO">
<contactref element="U1" pad="14"/>
<contactref element="GO" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="GO" pad="P$2"/>
<contactref element="PWR" pad="P$2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="22"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$9" pad="P$1"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="TCAMP" pad="P$3"/>
<contactref element="TCAMP" pad="P$2"/>
<contactref element="U$12" pad="P$1"/>
<contactref element="Q2" pad="1"/>
<contactref element="U$14" pad="P$2"/>
<contactref element="U$10" pad="LEFT"/>
<contactref element="U$15" pad="P$2"/>
<contactref element="U$13" pad="P$2"/>
<contactref element="U$16" pad="P$2"/>
<contactref element="U$17" pad="P$2"/>
</signal>
<signal name="EN">
<contactref element="U1" pad="17"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="LCDRS">
<contactref element="U1" pad="18"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="SENSEO">
<contactref element="TCAMP" pad="P$6"/>
<contactref element="TCAMP" pad="P$5"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="SENSE_M">
<contactref element="U$6" pad="P$2"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="TCAMP" pad="P$1"/>
</signal>
<signal name="SENSE_P">
<contactref element="U$4" pad="P$2"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="TCAMP" pad="P$8"/>
</signal>
<signal name="TC_P">
<contactref element="U$8" pad="P$1"/>
<contactref element="U$9" pad="P$2"/>
<contactref element="TCIN" pad="P$2"/>
</signal>
<signal name="TC_M">
<contactref element="TCIN" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="21"/>
<contactref element="U$10" pad="RIGHT"/>
<contactref element="U$15" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="1"/>
<contactref element="U$11" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$16"/>
<contactref element="U$12" pad="P$2"/>
</signal>
<signal name="DIM">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$13" pad="WIP"/>
</signal>
<signal name="N$6">
<contactref element="RELAY" pad="P$1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="RCTRL">
<contactref element="Q2" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="U$1" pad="P$14"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="U$1" pad="P$13"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="6"/>
<contactref element="U$1" pad="P$12"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="11"/>
<contactref element="U$1" pad="P$11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
