<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.254" x2="10.267" y2="-0.254" width="0" layer="20"/>
<wire x1="10.267" y1="-0.254" x2="10.267" y2="16.815" width="0" layer="20"/>
<wire x1="10.267" y1="16.815" x2="0" y2="16.815" width="0" layer="20"/>
<wire x1="0" y1="16.815" x2="0" y2="-0.254" width="0" layer="20"/>
<text>http://lachmoewe.net/brd/led</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-RGB-THRU">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-1.5X4.5">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED-RGB-THRU" value="LED-RGB-CA-THRUCLEAR">
<attribute name="PROD_ID" value="DIO-10631"/>
</element>
<element name="Q-RED" library="SparkFun-DiscreteSemi" package="SOT23" value="30V, 2.5A">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q-GREEN" library="SparkFun-DiscreteSemi" package="SOT23" value="30V, 2.5A">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q-BLUE" library="SparkFun-DiscreteSemi" package="SOT23" value="30V, 2.5A">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="R-RED" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R-GREEN" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R-BLUE" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="IC1" library="atmel" package="8S1" value="TINY13-20SSU">
<attribute name="OC_NEWARK" value="58M3771"/>
<attribute name="MPN" value="ATTINY13-20SSU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1455133"/>
</element>
<element name="VCC1" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="GND" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="VCC2" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="GND_" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="MISO" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="SCK" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="MOSI" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="SCK_" library="SparkFun-Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="C1" library="SparkFun-Passives" package="0805" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="1"/>
<contactref element="R-RED" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="4"/>
<contactref element="R-BLUE" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R-RED" pad="1"/>
<contactref element="Q-RED" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="3"/>
<contactref element="R-GREEN" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R-GREEN" pad="1"/>
<contactref element="Q-GREEN" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R-BLUE" pad="1"/>
<contactref element="Q-BLUE" pad="3"/>
</signal>
<signal name="GND">
<contactref element="Q-RED" pad="2"/>
<contactref element="Q-GREEN" pad="2"/>
<contactref element="Q-BLUE" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="GND" pad="P$1"/>
<contactref element="GND_" pad="P$1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="6"/>
<contactref element="MISO" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="7"/>
<contactref element="SCK" pad="P$1"/>
<contactref element="SCK_" pad="P$1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="1"/>
<contactref element="Q-BLUE" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="VCC1" pad="P$1"/>
<contactref element="VCC2" pad="P$1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="5"/>
<contactref element="MOSI" pad="P$1"/>
</signal>
<signal name="RED">
<contactref element="IC1" pad="2"/>
<contactref element="Q-RED" pad="1"/>
</signal>
<signal name="GREEN">
<contactref element="IC1" pad="3"/>
<contactref element="Q-GREEN" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
