<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="24.13" y1="0" x2="24.13" y2="15.23" width="0" layer="20"/>
<wire x1="24.13" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="10AWG">
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATT-" library="wirepad" package="10AWG" value="10AWG">
<attribute name="NAME"/>
</element>
<element name="BATT+" library="wirepad" package="10AWG" value="10AWG">
<attribute name="NAME"/>
</element>
<element name="VOUT" library="wirepad" package="10AWG" value="10AWG">
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="10AWG" value="10AWG">
<attribute name="NAME"/>
</element>
<element name="Q1" library="transistor-power" package="TO220BV" value="IRF740">
<attribute name="NAME"/>
</element>
<element name="IC1" library="microchip" package="TO92" value="TC54">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="47K">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="300K">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="300K">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="S"/>
<contactref element="BATT-" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="D"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="1"/>
<contactref element="Q1" pad="G"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="BATT+" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="VOUT" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
