<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="12.17100625" x2="1.27" y2="1.79605" width="0" layer="20"/>
<wire x1="1.27" y1="1.79605" x2="3.06605" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.06605" y1="0" x2="15.86996875" y2="0" width="0" layer="20"/>
<wire x1="15.86996875" y1="0" x2="17.45" y2="1.58003125" width="0" layer="20" curve="90"/>
<wire x1="17.45" y1="1.58003125" x2="17.45" y2="12.387996875" width="0" layer="20"/>
<wire x1="17.45" y1="12.387996875" x2="15.877996875" y2="13.96" width="0" layer="20" curve="90"/>
<wire x1="15.877996875" y1="13.96" x2="3.05899375" y2="13.96" width="0" layer="20"/>
<wire x1="3.05899375" y1="13.96" x2="1.27" y2="12.17100625" width="0" layer="20" curve="90"/>
<text>+</text>
<text>-</text>
<text>C</text>
<text>D</text>
<text>-</text>
<text>C</text>
<text>D</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;For debuggers and/or programemrs that support the Cortex Debug Connector (10-pin) interface.&lt;/p&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.digikey.com/product-detail/en/20021111-00010T4LF/609-3712-ND/2209072"&gt;Example Digikey Part&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X5-PTH-1.27MM" value="CORTEX_DEBUGPTH"/>
<element name="J2" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="9"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="DIO">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
