<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<circle x="38.1" y="39.37" radius="25.4" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="pmt">
<packages>
<package name="PMT_STRAIGHT_THROUGH">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-LARGE">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="pmt" package="PMT_STRAIGHT_THROUGH" value="PMT_SOCKET_STRAIGHT_NO_GATE"/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="HV_GND" library="wirepad" package="3,17/1,3" value=""/>
<element name="HV-" library="wirepad" package="3,17/1,3" value=""/>
<element name="A_GND" library="wirepad" package="3,17/1,3" value=""/>
<element name="ANODE" library="wirepad" package="3,17/1,3" value=""/>
<element name="R1" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R2" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R3" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R4" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R5" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R6" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R7" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R8" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R9" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R10" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R11" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R12" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R13" library="SparkFun-Passives" package="1/6W-RES" value=""/>
<element name="R14" library="SparkFun-Passives" package="AXIAL-0.6" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-LARGE" value=""/>
<element name="SHIELD" library="wirepad" package="3,17/1,3" value=""/>
</elements>
<signals>
<signal name="N$11">
<contactref element="U$1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="19"/>
<contactref element="R1" pad="1"/>
<contactref element="HV-" pad="1"/>
<contactref element="R14" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="15"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="14"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="5"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="13"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="12"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="7"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="11"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R13" pad="2"/>
<contactref element="A_GND" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="HV_GND" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="ANODE" pad="1"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$16">
<contactref element="R14" pad="P$1"/>
<contactref element="SHIELD" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
