<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-0.635" y1="8.5598" x2="12.0525" y2="8.5598" width="0.1524" layer="20"/>
<wire x1="12.0525" y1="8.5598" x2="12.0525" y2="26.66" width="0.1524" layer="20"/>
<wire x1="12.0525" y1="26.66" x2="-0.635" y2="26.66" width="0.1524" layer="20"/>
<wire x1="-0.635" y1="26.66" x2="-0.635" y2="8.5598" width="0.1524" layer="20"/>
<text>GND</text>
<text>3V3</text>
<text>VIN</text>
<text>MCP1703</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="jouni">
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="MICRO-USB5+4P-SMD-0.65-B">
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="Seeed-OPL-Diode">
<packages>
<package name="LED-0402">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AMS1117" library="SparkFun-PowerIC" package="SOT223" value="">
<attribute name="PROD_ID" value="VREG-08170"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="jouni" package="TO-92" value="MCP1700">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="jouni" package="SOT223" value="MCP1703">
<attribute name="VALUE"/>
</element>
<element name="USB1" library="jouni" package="MICRO-USB5+4P-SMD-0.65-B" value="ST-USB-001G">
<attribute name="MPN" value="ST-USB-001G"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="NAME"/>
</element>
<element name="PWR" library="Seeed-OPL-Diode" package="LED-0402" value="">
<attribute name="MPN" value="BL-HB337A-AV-TRB"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="1k">
<attribute name="NAME"/>
</element>
<element name="U$3" library="jouni" package="SOT23-3" value="MCP1703SOT23-3"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="1"/>
<contactref element="AMS1117" pad="1"/>
<contactref element="USB1" pad="5"/>
<contactref element="USB1" pad="S1"/>
<contactref element="USB1" pad="S2"/>
<contactref element="USB1" pad="S3"/>
<contactref element="USB1" pad="S4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="5V">
<contactref element="USB1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="AMS1117" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="PWR" pad="+"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="3V3">
<contactref element="U$2" pad="3"/>
<contactref element="AMS1117" pad="2"/>
<contactref element="AMS1117" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="PWR" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
