<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="7.9375" y1="-0.3175" x2="7.9375" y2="8.255" width="0.4064" layer="20"/>
<wire x1="7.9375" y1="8.255" x2="-0.3175" y2="8.255" width="0.4064" layer="20"/>
<wire x1="-0.3175" y1="8.255" x2="-0.3175" y2="-0.3175" width="0.4064" layer="20"/>
<wire x1="-0.3175" y1="-0.3175" x2="7.9375" y2="-0.3175" width="0.4064" layer="20"/>
<text>TPS799
(c) 2019 Paolo Iocco

[o] 3V0
[o] 3V3</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="paolo">
<description>Paolo's Library</description>
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TPS799" library="SparkFun-PowerIC" package="SOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN" library="testpad" package="P1-13" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="testpad" package="P1-13" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="testpad" package="P1-13" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C" library="paolo" package="C0805K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TPS799" pad="2"/>
<contactref element="GND" pad="TP"/>
<contactref element="C" pad="1"/>
</signal>
<signal name="IN">
<contactref element="TPS799" pad="1"/>
<contactref element="IN" pad="TP"/>
<contactref element="TPS799" pad="3"/>
</signal>
<signal name="OUT">
<contactref element="OUT" pad="TP"/>
<contactref element="TPS799" pad="5"/>
</signal>
<signal name="S$4">
<contactref element="TPS799" pad="4"/>
<contactref element="C" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
