<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<text>AMMETER SHIELD v2</text>
<wire x1="31.8516" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="31.8516" y2="17.78" width="0" layer="20"/>
<wire x1="31.8516" y1="17.78" x2="31.8516" y2="0" width="0" layer="20"/>
<text>BAT</text>
<text>GND</text>
<text>5V</text>
<text>3V3</text>
<text>4</text>
<text>14</text>
<text>15</text>
<text>27</text>
<text>26</text>
<text>25</text>
<text>SDA</text>
<text>33</text>
<text>SCL</text>
<text>5</text>
<text>18</text>
<text>19</text>
<text>23</text>
<text>32</text>
<text>26</text>
<text>3V3</text>
<text>4</text>
<text>27</text>
<text>14</text>
<text>GND</text>
<text>SDA</text>
<text>RST</text>
<text>33</text>
<text>SCL</text>
<text>5</text>
<text>18</text>
<text>RST</text>
<text>GND</text>
<text>25</text>
<text>15</text>
<text>BAT</text>
<text>5V</text>
<text>19</text>
<text>23</text>
<text>GND</text>
<text>32</text>
<text>https://swooby.com/PCBTP</text>
<text>+ve</text>
<text>load</text>
<text>-ve</text>
<text>A1  A0  ADDR
GND GND 0x40
GND VS+ 0x41
GND SDA 0x42
GND SCL 0x43
VS+ GND 0x44
VS+ VS+ 0x45
VS+ SDA 0x46
VS+ SCL 0x47
SDA GND 0x48
SDA VS+ 0x49
SDA SDA 0x4A
SDA SCL 0x4B
SCL GND 0x4C
SCL VS+ 0x4D
SCL SDA 0x4E
SCL SCL 0x4F</text>
<text>A0</text>
<text>A1</text>
</plain>
<libraries>
<library name="UnexpectedMaker">
<description>Generated from &lt;b&gt;WattsSegment_Display.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1X10_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOT23-8">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.ti.com/lit/ml/mpds099c/mpds099c.pdf</description>
</package>
<package name="0805-NO@1">
</package>
<package name="RESPACK_4X0603">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pv_jump-0r-smd">
<description>Soldering jumper and bridges</description>
<packages>
<package name="C0R-JMP_NONE">
<description>&lt;b&gt;0R Jumper Variant D&lt;/b&gt;&lt;p&gt;
Solder type</description>
</package>
</packages>
</library>
<library name="pv">
<packages>
<package name="RESC90152X87N">
<description>&lt;b&gt;FCSL 6036i 15290m&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LEFT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="RIGHT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U1" library="microbuilder" package="SOT23-8" value="INA219BIDCNT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805-NO@1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="5mm">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="microbuilder" package="RESPACK_4X0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JMPA0.0" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="VALUE"/>
</element>
<element name="JMPA0.1" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="VALUE"/>
</element>
<element name="JMPA1.0" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="VALUE"/>
</element>
<element name="JMPA1.1" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="VALUE"/>
</element>
<element name="R1" library="pv" package="RESC90152X87N" value="FCSL150R025FER">
<attribute name="DESCRIPTION" value="OHMITE - FCSL150R025FER - CURRENT SENSE RES, 0R025, 1%, 10 W, 6030"/>
<attribute name="HEIGHT" value="0.874mm"/>
<attribute name="MANUFACTURER_NAME" value="Ohmite"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FCSL150R025FER"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="RIGHT" pad="10"/>
<contactref element="LEFT" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="8"/>
<contactref element="R2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="JMPA0.0" pad="3"/>
<contactref element="JMPA1.0" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="LEFT" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="6"/>
<contactref element="R2" pad="5"/>
<contactref element="JMPA1.0" pad="1"/>
<contactref element="JMPA0.0" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="RIGHT" pad="9"/>
</signal>
<signal name="GND1">
</signal>
<signal name="DATA_OUT">
</signal>
<signal name="GPIO32">
<contactref element="RIGHT" pad="7"/>
</signal>
<signal name="GPIO33">
<contactref element="RIGHT" pad="8"/>
</signal>
<signal name="GPIO25">
<contactref element="LEFT" pad="10"/>
</signal>
<signal name="GPIO26">
<contactref element="LEFT" pad="9"/>
</signal>
<signal name="GPIO27">
<contactref element="LEFT" pad="8"/>
</signal>
<signal name="GPIO14">
<contactref element="LEFT" pad="6"/>
</signal>
<signal name="GPIO15">
<contactref element="LEFT" pad="7"/>
</signal>
<signal name="GPIO4">
<contactref element="LEFT" pad="5"/>
</signal>
<signal name="GPIO5">
<contactref element="RIGHT" pad="4"/>
</signal>
<signal name="GPIO18">
<contactref element="RIGHT" pad="3"/>
</signal>
<signal name="GPIO23">
<contactref element="RIGHT" pad="1"/>
</signal>
<signal name="GPIO19">
<contactref element="RIGHT" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="USB">
<contactref element="LEFT" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="RIGHT" pad="5"/>
<contactref element="R2" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="JMPA1.1" pad="1"/>
<contactref element="JMPA0.1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="RIGHT" pad="6"/>
<contactref element="R2" pad="3"/>
<contactref element="U1" pad="6"/>
<contactref element="JMPA1.1" pad="3"/>
<contactref element="JMPA0.1" pad="3"/>
</signal>
<signal name="VIN+">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VIN-">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="JMPA1.0" pad="2"/>
<contactref element="JMPA1.1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="A0">
<contactref element="JMPA0.0" pad="2"/>
<contactref element="JMPA0.1" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
