<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="40.564" y2="0" width="0.254" layer="20"/>
<wire x1="40.564" y1="0" x2="41.834" y2="1.27" width="0.254" layer="20" curve="90"/>
<wire x1="41.834" y1="1.27" x2="41.834" y2="28.184" width="0.254" layer="20"/>
<wire x1="41.834" y1="28.184" x2="40.564" y2="29.454" width="0.254" layer="20" curve="90"/>
<wire x1="40.564" y1="29.454" x2="1.27" y2="29.454" width="0.254" layer="20"/>
<wire x1="1.27" y1="29.454" x2="0" y2="28.184" width="0.254" layer="20" curve="90"/>
<wire x1="0" y1="28.184" x2="0" y2="1.27" width="0.254" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0.254" layer="20" curve="90"/>
<text>5V</text>
<text>S</text>
<hole x="39.624" y="27.178" drill="3.2"/>
<hole x="39.624" y="2.286" drill="3.2"/>
<text>v=5.0vdc
g=gnd
s=3.3vdc signal</text>
<text>L.C. ROSE 2017</text>
<text>G</text>
<text>DANGER</text>
<text>HIGH
VOLTAGE</text>
<hole x="2.286" y="27.178" drill="3.2"/>
<hole x="2.286" y="2.286" drill="3.2"/>
<text>JD-VCC</text>
<text>GND</text>
<text>5VDC</text>
<text>Opto Isolated Relay</text>
<text>R5 Pulldown if false triggering occurs</text>
<text>NC</text>
<text>NO</text>
<text>COM</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="G5LE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V ADC, Omron</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="1X04">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="AXIAL-0.1EZ">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="K1" library="relay" package="G5LE" value="G5LE">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904"/>
<element name="LED1" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="220">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="2.2k"/>
<element name="OK1" library="optocoupler" package="DIL04" value="PC817">
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707727"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="499">
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="TO92" value="2N3904"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1EZ" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-3" value="">
<attribute name="STOREFRONT_ID" value="PRT-08433"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="K1" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="GND">
<contactref element="T2" pad="3"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="P$1"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="K1" pad="P"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="S"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="OK1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="T2" pad="2"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="OK1" pad="2"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="OK1" pad="3"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="P$2"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="K1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="OK1" pad="4"/>
<contactref element="R2" pad="P$2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="T1" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="K1" pad="O"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="P$1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
