<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>GND</text>
<text>13</text>
<text>5V</text>
<wire x1="12.7" y1="11.303" x2="12.7" y2="0.508" width="0" layer="20"/>
<wire x1="12.7" y1="0.508" x2="12.192" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="12.192" y1="0" x2="0.762" y2="0" width="0" layer="20"/>
<wire x1="0.762" y1="0" x2="0" y2="0.508" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="0.508" x2="0" y2="11.303" width="0" layer="20"/>
<wire x1="0" y1="11.303" x2="0.635" y2="11.938" width="0" layer="20" curve="-90"/>
<wire x1="0.635" y1="11.938" x2="12.065" y2="11.938" width="0" layer="20"/>
<wire x1="12.065" y1="11.938" x2="12.7" y2="11.303" width="0" layer="20" curve="-90"/>
<text>5V</text>
<text>13</text>
<text>GND</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
</plain>
<libraries>
<library name="_c2h">
<packages>
<package name="0805-RES">
</package>
</packages>
</library>
<library name="Seeed-Transistor">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Diode">
<packages>
<package name="LL-34">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="_c2h" package="0805-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="Q1" library="Seeed-Transistor" package="SOT-23" value="BSS138">
<attribute name="MPN" value="CJ2302"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="Seeed-Diode" package="LL-34" value="1N4148">
<attribute name="MPN" value="1N4148"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05_LOCK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="IO13">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="5V">
<contactref element="J2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
