<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<board>
<plain>
<text>D2</text>
<text>RX</text>
<text>TX</text>
<text>D3</text>
<text>G</text>
<text>RST</text>
<text>5V</text>
<text>D5</text>
<text>D6</text>
<text>A0</text>
<text>3V3</text>
<text>D8</text>
<wire x1="25.4" y1="27.94" x2="25.4" y2="7.62" width="0.0254" layer="20"/>
<wire x1="25.4" y1="7.62" x2="0" y2="7.62" width="0.0254" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="27.94" width="0.0254" layer="20"/>
<wire x1="0" y1="27.94" x2="25.4" y2="27.94" width="0.0254" layer="20"/>
<text>RST</text>
<text>D5</text>
<text>D6</text>
<text>A0</text>
<text>3V3</text>
<text>D8</text>
<text>D2</text>
<text>RX</text>
<text>TX</text>
<text>D3</text>
<text>GND</text>
<text>5V</text>
<text>D1</text>
<text>D1</text>
<text>7 SEGMENT CLOCK SHIELD 1.1.1</text>
<text>D7</text>
<text>D0</text>
<text>D0</text>
<text>D5</text>
<text>D3</text>
<text>D4</text>
<text>GND</text>
<text>5V</text>
<text>D6(5V)</text>
<text>GND</text>
<text>5V</text>
<text>D2(5V)</text>
<text>74AHCT125</text>
<text>5V</text>
<text>GND</text>
<hole x="11.43" y="10.414" drill="3.2"/>
<hole x="15.24" y="25.4" drill="3.2"/>
<text>https://git.io/7s</text>
</plain>
<libraries>
<library name="freetronics-original">
<description>Spark Fun Electronics' preferred foot prints. We've spent an enormous amount of time creating and checking these footprints and parts.
If you enjoy using this library, please buy one of our products at http://www.sparkfun.com.
Please also note that we guarantee that there are some messed up footprints in this library.
We've tried to note which are proven and tested but by downloading this file, you acknowledge that you are using this file at your own risk.
We cannot be held responsible for faulty PCBs. Always check your parts against a 1:1 printout.

Licensing: CC v3.0 Share-Alike You are welcome to use this library for commercial purposes.
For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold.
We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H1" library="freetronics-original" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="H2" library="freetronics-original" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="5VDC" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="DIL14" value="74125N"/>
<element name="HOURS" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE"/>
</element>
<element name="MINS" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="GND">
<contactref element="H2" pad="7"/>
<contactref element="5VDC" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="9"/>
<contactref element="HOURS" pad="3"/>
<contactref element="MINS" pad="1"/>
</signal>
<signal name="D1">
<contactref element="H2" pad="3"/>
</signal>
<signal name="D2">
<contactref element="H2" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="D6">
<contactref element="H1" pad="5"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="D8">
<contactref element="H1" pad="7"/>
</signal>
<signal name="A0">
<contactref element="H1" pad="2"/>
</signal>
<signal name="D0">
<contactref element="H1" pad="3"/>
</signal>
<signal name="D3">
<contactref element="H2" pad="5"/>
</signal>
<signal name="D4">
<contactref element="H2" pad="6"/>
</signal>
<signal name="RX">
<contactref element="H2" pad="2"/>
</signal>
<signal name="TX">
<contactref element="H2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="H1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="H1" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="H2" pad="8"/>
<contactref element="5VDC" pad="1"/>
<contactref element="IC1" pad="14"/>
<contactref element="HOURS" pad="1"/>
<contactref element="MINS" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="6"/>
<contactref element="HOURS" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="11"/>
<contactref element="MINS" pad="2"/>
</signal>
<signal name="D5">
<contactref element="H1" pad="4"/>
</signal>
<signal name="D7">
<contactref element="H1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
