<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="35.56" y1="78.74" x2="92.71" y2="78.74" width="0.1524" layer="20"/>
<wire x1="92.71" y1="78.74" x2="92.71" y2="36.83" width="0.1524" layer="20"/>
<wire x1="92.71" y1="36.83" x2="35.56" y2="36.83" width="0.1524" layer="20"/>
<wire x1="35.56" y1="36.83" x2="35.56" y2="78.74" width="0.1524" layer="20"/>
<text>NIXIE POWER
SUPPLY</text>
<text>5 DEC 17</text>
<text>VERSION 1</text>
<text>180V</text>
</plain>
<libraries>
<library name="NIXIE">
<packages>
<package name="2917">
<description>Tantalum Capacitor&lt;br&gt;
http://datasheets.avx.com/TPS.pdf</description>
</package>
<package name="B82477R4104M100">
<description>100nH inductor&lt;br&gt;
https://en.tdk.eu/inf/30/ds/b82477r4.pdf</description>
</package>
<package name="STTH3R04U">
<description>ultrafast recovery diode&lt;br&gt;
http://www.st.com/content/ccc/resource/technical/document/datasheet/59/8d/cf/2a/cc/37/45/18/CD00199070.pdf/files/CD00199070.pdf/jcr:content/translations/en.CD00199070.pdf</description>
</package>
<package name="EB_G17">
<description>Electrolytic Capacitor&lt;br&gt;
https://industrial.panasonic.com/cdbs/www-data/pdf/RDE0000/ABA0000C1202.pdf</description>
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0805_A">
</package>
<package name="1206_A">
</package>
</packages>
</library>
<library name="PHOENIX">
<packages>
<package name="1729018">
<description>5mm 2 conductor&lt;br&gt;
https://media.digikey.com/pdf/Data%20Sheets/Phoenix%20Contact%20PDFs/1729018.pdf</description>
</package>
</packages>
</library>
<library name="User-Submitted">
<description>&lt;h3&gt;SparkFun User Contributed Parts&lt;/h3&gt;
In this library you'll find submitted parts from SparkFun users everywhere!&lt;br&gt;&lt;br&gt;
These are not necessarily parts we carry, but are parts that other users have determined function well with other parts in our libraries. Please keep in mind that it is the end user's responsibility to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;&lt;br&gt;
If you find these parts useful, please consider helping the open-source community by contributing your own through &lt;a href="https://github.com/sparkfun/SparkFun-Eagle-Libraries"&gt;GitHub.&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="MAXIM">
<packages>
<package name="SOIC-N-8">
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0805">
</package>
<package name="2512">
<description>https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf</description>
</package>
</packages>
</library>
<library name="CUI">
<packages>
<package name="PJ-102AH">
<description>Standard Power Jack.
http://www.cui.com/product/resource/pj-102ah.pdf</description>
</package>
</packages>
</library>
<library name="Bourns">
<packages>
<package name="3214W">
<description>3214W Top Adjust&lt;br&gt;
http://www.bourns.com/docs/Product-Datasheets/3214.pdf</description>
</package>
</packages>
</library>
<library name="3M">
<packages>
<package name="SJ-5003">
<description>Black 0.44" diameter 0.097" (5mm) thick</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="NIXIE" package="2917" value="100u"/>
<element name="C2" library="KEMET" package="0805_A" value="100n"/>
<element name="C3" library="KEMET" package="0805_A" value="100n"/>
<element name="L1" library="NIXIE" package="B82477R4104M100" value=""/>
<element name="POWER" library="PHOENIX" package="1729018" value="MO2"/>
<element name="Q1" library="User-Submitted" package="TO220V" value="MOSFET-PCHANNELFQP27P06">
<attribute name="NAME"/>
</element>
<element name="SHDN" library="PHOENIX" package="1729018" value="MO2"/>
<element name="U$1" library="MAXIM" package="SOIC-N-8" value="MAX1771"/>
<element name="D1" library="NIXIE" package="STTH3R04U" value="DIODE"/>
<element name="V+" library="PHOENIX" package="1729018" value="MO2"/>
<element name="VOUT" library="PHOENIX" package="1729018" value="MO2"/>
<element name="C5" library="NIXIE" package="2917" value="10u"/>
<element name="C4" library="NIXIE" package="EB_G17" value=""/>
<element name="R1" library="Stackpole" package="2512" value="1M5"/>
<element name="R2" library="Stackpole" package="0805" value="10K"/>
<element name="C6" library="KEMET" package="1206_A" value="100n"/>
<element name="V1" library="CUI" package="PJ-102AH" value="POWER_JACK"/>
<element name="P1" library="Bourns" package="3214W" value=""/>
<element name="RSENSE" library="Stackpole" package="2512" value="0R050"/>
<element name="U$2" library="3M" package="SJ-5003" value=""/>
<element name="U$3" library="3M" package="SJ-5003" value=""/>
<element name="U$4" library="3M" package="SJ-5003" value=""/>
<element name="U$5" library="3M" package="SJ-5003" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="V+" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="C5" pad="A"/>
</signal>
<signal name="GND">
<contactref element="V+" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="K"/>
<contactref element="POWER" pad="2"/>
<contactref element="VOUT" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="7"/>
<contactref element="C5" pad="K"/>
<contactref element="C4" pad="K"/>
<contactref element="R2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="V1" pad="2"/>
<contactref element="RSENSE" pad="A"/>
<contactref element="SHDN" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="POWER">
<contactref element="C1" pad="A"/>
<contactref element="POWER" pad="1"/>
<contactref element="L1" pad="P$1"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="EXT">
<contactref element="Q1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="CS">
<contactref element="Q1" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="RSENSE" pad="B"/>
</signal>
<signal name="N$6">
<contactref element="SHDN" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="K"/>
<contactref element="VOUT" pad="2"/>
<contactref element="C4" pad="A"/>
<contactref element="R1" pad="B"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="Q1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="MOPV">
<contactref element="U$1" pad="3"/>
<contactref element="R1" pad="A"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="SW">
<contactref element="V1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="P1" pad="1"/>
<contactref element="P1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
