<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="34.29" y1="59.69" x2="54.61" y2="59.69" width="0" layer="20"/>
<wire x1="54.61" y1="59.69" x2="54.61" y2="21.59" width="0" layer="20"/>
<wire x1="54.61" y1="21.59" x2="34.29" y2="21.59" width="0" layer="20"/>
<wire x1="34.29" y1="21.59" x2="34.29" y2="59.69" width="0" layer="20"/>
<text>Multwatt15 BOB</text>
<text>TDA7376B</text>
<text>12Feb2015</text>
<text>v1</text>
<text>15</text>
<text>1</text>
</plain>
<libraries>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="MULTIWATT_15">
<description>Multiwatt 15 V footprint
From the TDA7297 Datasheet
Center hole should be about 0.75 inches above board surface</description>
</package>
<package name="HEAT_SINK_R_SERIES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ERIC" package="MULTIWATT_15" value="TDA7376B"/>
<element name="JP1" library="SparkFun-Connectors" package="1X15" value="M15"/>
<element name="U$2" library="ERIC" package="HEAT_SINK_R_SERIES" value="HEAT_SINKR_SERIES"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="11"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="12"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="13"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="14"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="15"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="P$1">
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="P$2">
<contactref element="U$2" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
