<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="66.04" y2="0" width="0.4064" layer="20"/>
<wire x1="66.04" y1="0" x2="66.04" y2="2.54" width="0.4064" layer="20"/>
<wire x1="66.04" y1="2.54" x2="68.58" y2="5.08" width="0.4064" layer="20"/>
<wire x1="68.58" y1="5.08" x2="68.58" y2="37.846" width="0.4064" layer="20"/>
<wire x1="68.58" y1="37.846" x2="66.04" y2="40.386" width="0.4064" layer="20"/>
<wire x1="66.04" y1="40.386" x2="66.04" y2="51.816" width="0.4064" layer="20"/>
<wire x1="66.04" y1="51.816" x2="64.516" y2="53.34" width="0.4064" layer="20"/>
<wire x1="64.516" y1="53.34" x2="0" y2="53.34" width="0.4064" layer="20"/>
<wire x1="0" y1="53.34" x2="0" y2="0" width="0.4064" layer="20"/>
<text>DI</text>
<text>5V</text>
<text>GND</text>
<text>DO</text>
<text>NeoPixelRGBW</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>3.V</text>
<text>5V</text>
<text>GND</text>
<text>CLK</text>
<text>DO</text>
<text>DI</text>
<text>CS</text>
<text>CD</text>
<text>adafruit SD Card Reader</text>
<text>5V RELAY</text>
<text>Michael</text>
<text>Bennett</text>
<text>NeoPixel STRIPS</text>
<text>5V</text>
<text>GND</text>
<text>[USE</text>
<text>AMP</text>
<text>BRAKE</text>
<text>RESET</text>
<text>F-150 AUXILIARY</text>
<text>CONTROLLER v1.0</text>
<text>REAR</text>
<text>FRONT</text>
<text>R</text>
<text>G</text>
<text>B</text>
<text>R</text>
<text>G</text>
<text>B</text>
<text>SW1</text>
<text>5V</text>
<text>SW2</text>
<text>5V</text>
<text>BUTTON</text>
<text>(DRIVER)</text>
<text>BUTTON</text>
<text>(PASSENGER)</text>
<text>[EXTERNAL]</text>
<text>POWER]</text>
<text>BYPASS</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_LONGPAD">
<description>&lt;h3&gt;Plated Through Hole - Long Pad&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-5MM-10MM">
<description>5 mm spaced PTHs in 10 mm diameter silk ring</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANALOG_IN" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BUTTON_1" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BUTTON_2" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-5MM-10MM" value="1000uF">
<attribute name="PROD_ID" value="CAP-09538"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="DIGITAL_1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DIGITAL_2" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FD" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FP" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RD" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_POWER" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PARKING_BRAKE" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PBRAKE2" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PBRAKE_1" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY_1" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY_2" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REMOTE" library="SparkFun-Connectors" package="1X01_LONGPAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SD_CARD" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="EXT_GND">
<contactref element="LED_POWER" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="FD" pad="3"/>
<contactref element="FP" pad="3"/>
<contactref element="RD" pad="3"/>
<contactref element="RP" pad="3"/>
</signal>
<signal name="EXT_5V">
<contactref element="FD" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="LED_POWER" pad="1"/>
<contactref element="FP" pad="2"/>
<contactref element="RD" pad="2"/>
<contactref element="RP" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="FD" pad="4"/>
<contactref element="FP" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="FP" pad="4"/>
<contactref element="RD" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="RD" pad="4"/>
<contactref element="RP" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="FD" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="POWER" pad="2"/>
<contactref element="POWER" pad="3"/>
<contactref element="SD_CARD" pad="3"/>
<contactref element="RELAY_1" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="POWER" pad="4"/>
<contactref element="SD_CARD" pad="1"/>
<contactref element="BUTTON_1" pad="3"/>
<contactref element="BUTTON_1" pad="5"/>
<contactref element="BUTTON_2" pad="3"/>
<contactref element="BUTTON_2" pad="5"/>
</signal>
<signal name="CLK">
<contactref element="DIGITAL_2" pad="6"/>
<contactref element="SD_CARD" pad="4"/>
</signal>
<signal name="SD_DO">
<contactref element="DIGITAL_2" pad="5"/>
<contactref element="SD_CARD" pad="5"/>
</signal>
<signal name="SD_IN">
<contactref element="DIGITAL_2" pad="4"/>
<contactref element="SD_CARD" pad="6"/>
</signal>
<signal name="CS">
<contactref element="DIGITAL_2" pad="3"/>
<contactref element="SD_CARD" pad="7"/>
</signal>
<signal name="NEO_DO">
<contactref element="R1" pad="P$1"/>
<contactref element="DIGITAL_2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="PARKING_BRAKE" pad="2"/>
<contactref element="PBRAKE_1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="PBRAKE2" pad="1"/>
<contactref element="PARKING_BRAKE" pad="1"/>
</signal>
<signal name="PBRAKE">
<contactref element="RELAY_2" pad="1"/>
<contactref element="DIGITAL_2" pad="1"/>
</signal>
<signal name="SW1">
<contactref element="DIGITAL_1" pad="8"/>
<contactref element="BUTTON_1" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="SW2">
<contactref element="DIGITAL_1" pad="2"/>
<contactref element="BUTTON_2" pad="1"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="LED_RED">
<contactref element="BUTTON_1" pad="2"/>
<contactref element="BUTTON_2" pad="2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="LED_GRN">
<contactref element="BUTTON_2" pad="4"/>
<contactref element="BUTTON_1" pad="4"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="LED_BLU">
<contactref element="BUTTON_1" pad="6"/>
<contactref element="BUTTON_2" pad="6"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="RMOTE">
<contactref element="DIGITAL_1" pad="5"/>
<contactref element="REMOTE" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="DIGITAL_1" pad="7"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="P$2"/>
<contactref element="DIGITAL_1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="P$2"/>
<contactref element="DIGITAL_1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="POWER" pad="6"/>
<contactref element="S1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
