<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0.2032" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="17.78" width="0.2032" layer="20"/>
<wire x1="17.78" y1="17.78" x2="0" y2="17.78" width="0.2032" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0.2032" layer="20"/>
<text>Noid Driver V0.01
CO2REG.COM</text>
<text>raw</text>
<text>gnd</text>
<text>in</text>
<text>sol-</text>
<text>sol+</text>
<text>Gate Volts: 3.75
Watts: 45</text>
<text>pin 2 input</text>
<text>Max 1 amp
continuous</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
<package name="1X02">
</package>
<package name="1X07">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO220S">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead molded, vertical</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="SparkFun" package="TO220V" value="RFP30N6LE"/>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO220S" value="BYW29"/>
<element name="JP1" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="Q1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="CONTROL">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="JP8" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="HIGH-CURRENT">
<contactref element="Q1" pad="2"/>
<contactref element="JP8" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
