<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="63.5" width="0.3" layer="20"/>
<wire x1="0" y1="63.5" x2="41.91" y2="63.5" width="0.3" layer="20"/>
<wire x1="41.91" y1="63.5" x2="41.91" y2="0" width="0.3" layer="20"/>
<wire x1="41.91" y1="0" x2="0" y2="0" width="0.3" layer="20"/>
<text>AND TRAINING KIT</text>
<text>V1.0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
<library name="User-Submitted">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find submitted parts from SparkFun users everywhere!&lt;br&gt;&lt;br&gt;
These are not necessarily parts we carry, but are parts that other users have determined function well with other parts in our libraries. Please keep in mind that it is the end user's responsibility to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;&lt;br&gt;
If you find these parts useful, please consider helping the open-source community by contributing your own through GitHub. https://github.com/sparkfun/SparkFun-Eagle-Libraries
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CCTTV1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="A-IN-1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A-IN-2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B-IN-1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B-IN-2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C-IN-1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C-IN-2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D-IN-1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D-IN-2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND-IN" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="74xx-eu" package="DIL14" value="74LS08N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED10" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED12" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.1" value="1k">
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="S-IN" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-OUT" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="User-Submitted" package="CCTTV1" value="CCTT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="7"/>
<contactref element="GND-IN" pad="1"/>
<contactref element="GND-OUT" pad="1"/>
<contactref element="LED9" pad="K"/>
<contactref element="LED10" pad="K"/>
<contactref element="LED11" pad="K"/>
<contactref element="LED12" pad="K"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="LED6" pad="K"/>
<contactref element="LED7" pad="K"/>
<contactref element="LED8" pad="K"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="14"/>
<contactref element="S-IN" pad="1"/>
<contactref element="S-OUT" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="P$1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="P$1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="P$1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="P$1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="P$1"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="P$1"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="P$1"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="P$1"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="P$1"/>
<contactref element="LED11" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R12" pad="P$1"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="AI1">
<contactref element="IC1" pad="1"/>
<contactref element="A-IN-1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="AI2">
<contactref element="IC1" pad="2"/>
<contactref element="A-IN-2" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="BI1">
<contactref element="IC1" pad="4"/>
<contactref element="B-IN-1" pad="1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="BI2">
<contactref element="IC1" pad="5"/>
<contactref element="B-IN-2" pad="1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="CI1">
<contactref element="IC1" pad="9"/>
<contactref element="C-IN-1" pad="1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="CI2">
<contactref element="IC1" pad="10"/>
<contactref element="C-IN-2" pad="1"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="DI1">
<contactref element="IC1" pad="12"/>
<contactref element="D-IN-1" pad="1"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="DI2">
<contactref element="IC1" pad="13"/>
<contactref element="D-IN-2" pad="1"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="A-OUT">
<contactref element="IC1" pad="3"/>
<contactref element="A-OUT" pad="1"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="B-OUT">
<contactref element="IC1" pad="6"/>
<contactref element="B-OUT" pad="1"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="C-OUT">
<contactref element="IC1" pad="8"/>
<contactref element="C-OUT" pad="1"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="D-OUT">
<contactref element="IC1" pad="11"/>
<contactref element="D-OUT" pad="1"/>
<contactref element="R12" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
